# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F429BETx
GenF4.menu.pnum.GENERIC_F429BETX=Generic F429BETx
GenF4.menu.pnum.GENERIC_F429BETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F429BETX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429BETX.build.board=GENERIC_F429BETX
GenF4.menu.pnum.GENERIC_F429BETX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429BETX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F429BETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F429BGTx
GenF4.menu.pnum.GENERIC_F429BGTX=Generic F429BGTx
GenF4.menu.pnum.GENERIC_F429BGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F429BGTX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429BGTX.build.board=GENERIC_F429BGTX
GenF4.menu.pnum.GENERIC_F429BGTX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429BGTX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F429BGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F429BITx
GenF4.menu.pnum.GENERIC_F429BITX=Generic F429BITx
GenF4.menu.pnum.GENERIC_F429BITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F429BITX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429BITX.build.board=GENERIC_F429BITX
GenF4.menu.pnum.GENERIC_F429BITX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429BITX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F429BITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F429NEHx
GenF4.menu.pnum.GENERIC_F429NEHX=Generic F429NEHx
GenF4.menu.pnum.GENERIC_F429NEHX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F429NEHX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429NEHX.build.board=GENERIC_F429NEHX
GenF4.menu.pnum.GENERIC_F429NEHX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429NEHX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F429NEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F429NGHx
GenF4.menu.pnum.GENERIC_F429NGHX=Generic F429NGHx
GenF4.menu.pnum.GENERIC_F429NGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F429NGHX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429NGHX.build.board=GENERIC_F429NGHX
GenF4.menu.pnum.GENERIC_F429NGHX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429NGHX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F429NGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F429NIHx
GenF4.menu.pnum.GENERIC_F429NIHX=Generic F429NIHx
GenF4.menu.pnum.GENERIC_F429NIHX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F429NIHX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429NIHX.build.board=GENERIC_F429NIHX
GenF4.menu.pnum.GENERIC_F429NIHX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429NIHX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F429NIHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F439BGTx
GenF4.menu.pnum.GENERIC_F439BGTX=Generic F439BGTx
GenF4.menu.pnum.GENERIC_F439BGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F439BGTX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F439BGTX.build.board=GENERIC_F439BGTX
GenF4.menu.pnum.GENERIC_F439BGTX.build.product_line=STM32F439xx
GenF4.menu.pnum.GENERIC_F439BGTX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F439BGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F439.svd

# Generic F439BITx
GenF4.menu.pnum.GENERIC_F439BITX=Generic F439BITx
GenF4.menu.pnum.GENERIC_F439BITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F439BITX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F439BITX.build.board=GENERIC_F439BITX
GenF4.menu.pnum.GENERIC_F439BITX.build.product_line=STM32F439xx
GenF4.menu.pnum.GENERIC_F439BITX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F439BITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F439.svd

# Generic F439NGHx
GenF4.menu.pnum.GENERIC_F439NGHX=Generic F439NGHx
GenF4.menu.pnum.GENERIC_F439NGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F439NGHX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F439NGHX.build.board=GENERIC_F439NGHX
GenF4.menu.pnum.GENERIC_F439NGHX.build.product_line=STM32F439xx
GenF4.menu.pnum.GENERIC_F439NGHX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F439NGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F439.svd

# Generic F439NIHx
GenF4.menu.pnum.GENERIC_F439NIHX=Generic F439NIHx
GenF4.menu.pnum.GENERIC_F439NIHX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F439NIHX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F439NIHX.build.board=GENERIC_F439NIHX
GenF4.menu.pnum.GENERIC_F439NIHX.build.product_line=STM32F439xx
GenF4.menu.pnum.GENERIC_F439NIHX.build.variant=STM32F4xx/F429B(E-G-I)T_F429N(E-G-I)H_F439B(G-I)T_F439N(G-I)H
GenF4.menu.pnum.GENERIC_F439NIHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F439.svd

