# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L072CBTx
GenL0.menu.pnum.GENERIC_L072CBTX=Generic L072CBTx
GenL0.menu.pnum.GENERIC_L072CBTX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L072CBTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072CBTX.build.board=GENERIC_L072CBTX
GenL0.menu.pnum.GENERIC_L072CBTX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072CBTX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L072CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072CZTx
GenL0.menu.pnum.GENERIC_L072CZTX=Generic L072CZTx
GenL0.menu.pnum.GENERIC_L072CZTX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072CZTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072CZTX.build.board=GENERIC_L072CZTX
GenL0.menu.pnum.GENERIC_L072CZTX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072CZTX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L072CZTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072CBUx
GenL0.menu.pnum.GENERIC_L072CBUX=Generic L072CBUx
GenL0.menu.pnum.GENERIC_L072CBUX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L072CBUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072CBUX.build.board=GENERIC_L072CBUX
GenL0.menu.pnum.GENERIC_L072CBUX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072CBUX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L072CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072CZUx
GenL0.menu.pnum.GENERIC_L072CZUX=Generic L072CZUx
GenL0.menu.pnum.GENERIC_L072CZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072CZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072CZUX.build.board=GENERIC_L072CZUX
GenL0.menu.pnum.GENERIC_L072CZUX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072CZUX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L072CZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L073CBTx
GenL0.menu.pnum.GENERIC_L073CBTX=Generic L073CBTx
GenL0.menu.pnum.GENERIC_L073CBTX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L073CBTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073CBTX.build.board=GENERIC_L073CBTX
GenL0.menu.pnum.GENERIC_L073CBTX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073CBTX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L073CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L073CZTx
GenL0.menu.pnum.GENERIC_L073CZTX=Generic L073CZTx
GenL0.menu.pnum.GENERIC_L073CZTX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L073CZTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073CZTX.build.board=GENERIC_L073CZTX
GenL0.menu.pnum.GENERIC_L073CZTX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073CZTX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L073CZTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L073CBUx
GenL0.menu.pnum.GENERIC_L073CBUX=Generic L073CBUx
GenL0.menu.pnum.GENERIC_L073CBUX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L073CBUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073CBUX.build.board=GENERIC_L073CBUX
GenL0.menu.pnum.GENERIC_L073CBUX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073CBUX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L073CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L073CZUx
GenL0.menu.pnum.GENERIC_L073CZUX=Generic L073CZUx
GenL0.menu.pnum.GENERIC_L073CZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L073CZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073CZUX.build.board=GENERIC_L073CZUX
GenL0.menu.pnum.GENERIC_L073CZUX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073CZUX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L073CZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L082CZUx
GenL0.menu.pnum.GENERIC_L082CZUX=Generic L082CZUx
GenL0.menu.pnum.GENERIC_L082CZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L082CZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L082CZUX.build.board=GENERIC_L082CZUX
GenL0.menu.pnum.GENERIC_L082CZUX.build.product_line=STM32L082xx
GenL0.menu.pnum.GENERIC_L082CZUX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L082CZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L083CBTx
GenL0.menu.pnum.GENERIC_L083CBTX=Generic L083CBTx
GenL0.menu.pnum.GENERIC_L083CBTX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L083CBTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L083CBTX.build.board=GENERIC_L083CBTX
GenL0.menu.pnum.GENERIC_L083CBTX.build.product_line=STM32L083xx
GenL0.menu.pnum.GENERIC_L083CBTX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L083CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L083CZTx
GenL0.menu.pnum.GENERIC_L083CZTX=Generic L083CZTx
GenL0.menu.pnum.GENERIC_L083CZTX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L083CZTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L083CZTX.build.board=GENERIC_L083CZTX
GenL0.menu.pnum.GENERIC_L083CZTX.build.product_line=STM32L083xx
GenL0.menu.pnum.GENERIC_L083CZTX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L083CZTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L083CZUx
GenL0.menu.pnum.GENERIC_L083CZUX=Generic L083CZUx
GenL0.menu.pnum.GENERIC_L083CZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L083CZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L083CZUX.build.board=GENERIC_L083CZUX
GenL0.menu.pnum.GENERIC_L083CZUX.build.product_line=STM32L083xx
GenL0.menu.pnum.GENERIC_L083CZUX.build.variant=STM32L0xx/L072C(B-Z)(T-U)_L073C(B-Z)(T-U)_L082CZU_L083CBT_L083CZ(T-U)
GenL0.menu.pnum.GENERIC_L083CZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

