# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U575RGTx
GenU5.menu.pnum.GENERIC_U575RGTX=Generic U575RGTx
GenU5.menu.pnum.GENERIC_U575RGTX.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575RGTX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575RGTX.build.board=GENERIC_U575RGTX
GenU5.menu.pnum.GENERIC_U575RGTX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575RGTX.build.variant=STM32U5xx/U575R(G-I)T_U585RIT
GenU5.menu.pnum.GENERIC_U575RGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575RITx
GenU5.menu.pnum.GENERIC_U575RITX=Generic U575RITx
GenU5.menu.pnum.GENERIC_U575RITX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575RITX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575RITX.build.board=GENERIC_U575RITX
GenU5.menu.pnum.GENERIC_U575RITX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575RITX.build.variant=STM32U5xx/U575R(G-I)T_U585RIT
GenU5.menu.pnum.GENERIC_U575RITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U585RITx
GenU5.menu.pnum.GENERIC_U585RITX=Generic U585RITx
GenU5.menu.pnum.GENERIC_U585RITX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585RITX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585RITX.build.board=GENERIC_U585RITX
GenU5.menu.pnum.GENERIC_U585RITX.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585RITX.build.variant=STM32U5xx/U575R(G-I)T_U585RIT
GenU5.menu.pnum.GENERIC_U585RITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

