# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F407IEHx
GenF4.menu.pnum.GENERIC_F407IEHX=Generic F407IEHx
GenF4.menu.pnum.GENERIC_F407IEHX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F407IEHX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F407IEHX.build.board=GENERIC_F407IEHX
GenF4.menu.pnum.GENERIC_F407IEHX.build.product_line=STM32F407xx
GenF4.menu.pnum.GENERIC_F407IEHX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F407IEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F407.svd

# Generic F407IGHx
GenF4.menu.pnum.GENERIC_F407IGHX=Generic F407IGHx
GenF4.menu.pnum.GENERIC_F407IGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F407IGHX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F407IGHX.build.board=GENERIC_F407IGHX
GenF4.menu.pnum.GENERIC_F407IGHX.build.product_line=STM32F407xx
GenF4.menu.pnum.GENERIC_F407IGHX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F407IGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F407.svd

# Generic F407IETx
GenF4.menu.pnum.GENERIC_F407IETX=Generic F407IETx
GenF4.menu.pnum.GENERIC_F407IETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F407IETX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F407IETX.build.board=GENERIC_F407IETX
GenF4.menu.pnum.GENERIC_F407IETX.build.product_line=STM32F407xx
GenF4.menu.pnum.GENERIC_F407IETX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F407IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F407.svd

# Generic F407IGTx
GenF4.menu.pnum.GENERIC_F407IGTX=Generic F407IGTx
GenF4.menu.pnum.GENERIC_F407IGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F407IGTX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F407IGTX.build.board=GENERIC_F407IGTX
GenF4.menu.pnum.GENERIC_F407IGTX.build.product_line=STM32F407xx
GenF4.menu.pnum.GENERIC_F407IGTX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F407IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F407.svd

# Generic F417IEHx
GenF4.menu.pnum.GENERIC_F417IEHX=Generic F417IEHx
GenF4.menu.pnum.GENERIC_F417IEHX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F417IEHX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F417IEHX.build.board=GENERIC_F417IEHX
GenF4.menu.pnum.GENERIC_F417IEHX.build.product_line=STM32F417xx
GenF4.menu.pnum.GENERIC_F417IEHX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F417IEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F417.svd

# Generic F417IGHx
GenF4.menu.pnum.GENERIC_F417IGHX=Generic F417IGHx
GenF4.menu.pnum.GENERIC_F417IGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F417IGHX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F417IGHX.build.board=GENERIC_F417IGHX
GenF4.menu.pnum.GENERIC_F417IGHX.build.product_line=STM32F417xx
GenF4.menu.pnum.GENERIC_F417IGHX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F417IGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F417.svd

# Generic F417IETx
GenF4.menu.pnum.GENERIC_F417IETX=Generic F417IETx
GenF4.menu.pnum.GENERIC_F417IETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F417IETX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F417IETX.build.board=GENERIC_F417IETX
GenF4.menu.pnum.GENERIC_F417IETX.build.product_line=STM32F417xx
GenF4.menu.pnum.GENERIC_F417IETX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F417IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F417.svd

# Generic F417IGTx
GenF4.menu.pnum.GENERIC_F417IGTX=Generic F417IGTx
GenF4.menu.pnum.GENERIC_F417IGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F417IGTX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F417IGTX.build.board=GENERIC_F417IGTX
GenF4.menu.pnum.GENERIC_F417IGTX.build.product_line=STM32F417xx
GenF4.menu.pnum.GENERIC_F417IGTX.build.variant=STM32F4xx/F407I(E-G)(H-T)_F417I(E-G)(H-T)
GenF4.menu.pnum.GENERIC_F417IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F417.svd

