# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U575ZGTxQ
GenU5.menu.pnum.GENERIC_U575ZGTXQ=Generic U575ZGTxQ
GenU5.menu.pnum.GENERIC_U575ZGTXQ.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575ZGTXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575ZGTXQ.build.board=GENERIC_U575ZGTXQ
GenU5.menu.pnum.GENERIC_U575ZGTXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575ZGTXQ.build.variant=STM32U5xx/U575Z(G-I)TxQ_U585ZITxQ
GenU5.menu.pnum.GENERIC_U575ZGTXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575ZITxQ
GenU5.menu.pnum.GENERIC_U575ZITXQ=Generic U575ZITxQ
GenU5.menu.pnum.GENERIC_U575ZITXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575ZITXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575ZITXQ.build.board=GENERIC_U575ZITXQ
GenU5.menu.pnum.GENERIC_U575ZITXQ.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575ZITXQ.build.variant=STM32U5xx/U575Z(G-I)TxQ_U585ZITxQ
GenU5.menu.pnum.GENERIC_U575ZITXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U585ZITxQ
GenU5.menu.pnum.GENERIC_U585ZITXQ=Generic U585ZITxQ
GenU5.menu.pnum.GENERIC_U585ZITXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585ZITXQ.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585ZITXQ.build.board=GENERIC_U585ZITXQ
GenU5.menu.pnum.GENERIC_U585ZITXQ.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585ZITXQ.build.variant=STM32U5xx/U575Z(G-I)TxQ_U585ZITxQ
GenU5.menu.pnum.GENERIC_U585ZITXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

