# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F407ZETx
GenF4.menu.pnum.GENERIC_F407ZETX=Generic F407ZETx
GenF4.menu.pnum.GENERIC_F407ZETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F407ZETX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F407ZETX.build.board=GENERIC_F407ZETX
GenF4.menu.pnum.GENERIC_F407ZETX.build.product_line=STM32F407xx
GenF4.menu.pnum.GENERIC_F407ZETX.build.variant=STM32F4xx/F407Z(E-G)T_F417Z(E-G)T
GenF4.menu.pnum.GENERIC_F407ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F407.svd

# Generic F407ZGTx
GenF4.menu.pnum.GENERIC_F407ZGTX=Generic F407ZGTx
GenF4.menu.pnum.GENERIC_F407ZGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F407ZGTX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F407ZGTX.build.board=GENERIC_F407ZGTX
GenF4.menu.pnum.GENERIC_F407ZGTX.build.product_line=STM32F407xx
GenF4.menu.pnum.GENERIC_F407ZGTX.build.variant=STM32F4xx/F407Z(E-G)T_F417Z(E-G)T
GenF4.menu.pnum.GENERIC_F407ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F407.svd

# Generic F417ZETx
GenF4.menu.pnum.GENERIC_F417ZETX=Generic F417ZETx
GenF4.menu.pnum.GENERIC_F417ZETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F417ZETX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F417ZETX.build.board=GENERIC_F417ZETX
GenF4.menu.pnum.GENERIC_F417ZETX.build.product_line=STM32F417xx
GenF4.menu.pnum.GENERIC_F417ZETX.build.variant=STM32F4xx/F407Z(E-G)T_F417Z(E-G)T
GenF4.menu.pnum.GENERIC_F417ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F417.svd

# Generic F417ZGTx
GenF4.menu.pnum.GENERIC_F417ZGTX=Generic F417ZGTx
GenF4.menu.pnum.GENERIC_F417ZGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F417ZGTX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F417ZGTX.build.board=GENERIC_F417ZGTX
GenF4.menu.pnum.GENERIC_F417ZGTX.build.product_line=STM32F417xx
GenF4.menu.pnum.GENERIC_F417ZGTX.build.variant=STM32F4xx/F407Z(E-G)T_F417Z(E-G)T
GenF4.menu.pnum.GENERIC_F417ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F417.svd

