# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F413VGHx
GenF4.menu.pnum.GENERIC_F413VGHX=Generic F413VGHx
GenF4.menu.pnum.GENERIC_F413VGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F413VGHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F413VGHX.build.board=GENERIC_F413VGHX
GenF4.menu.pnum.GENERIC_F413VGHX.build.product_line=STM32F413xx
GenF4.menu.pnum.GENERIC_F413VGHX.build.variant=STM32F4xx/F413V(G-H)H_F423VHH
GenF4.menu.pnum.GENERIC_F413VGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F413.svd

# Generic F413VHHx
GenF4.menu.pnum.GENERIC_F413VHHX=Generic F413VHHx
GenF4.menu.pnum.GENERIC_F413VHHX.upload.maximum_size=1572864
GenF4.menu.pnum.GENERIC_F413VHHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F413VHHX.build.board=GENERIC_F413VHHX
GenF4.menu.pnum.GENERIC_F413VHHX.build.product_line=STM32F413xx
GenF4.menu.pnum.GENERIC_F413VHHX.build.variant=STM32F4xx/F413V(G-H)H_F423VHH
GenF4.menu.pnum.GENERIC_F413VHHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F413.svd

# Generic F423VHHx
GenF4.menu.pnum.GENERIC_F423VHHX=Generic F423VHHx
GenF4.menu.pnum.GENERIC_F423VHHX.upload.maximum_size=1572864
GenF4.menu.pnum.GENERIC_F423VHHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F423VHHX.build.board=GENERIC_F423VHHX
GenF4.menu.pnum.GENERIC_F423VHHX.build.product_line=STM32F423xx
GenF4.menu.pnum.GENERIC_F423VHHX.build.variant=STM32F4xx/F413V(G-H)H_F423VHH
GenF4.menu.pnum.GENERIC_F423VHHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F423.svd

