# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F722ICKx
GenF7.menu.pnum.GENERIC_F722ICKX=Generic F722ICKx
GenF7.menu.pnum.GENERIC_F722ICKX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F722ICKX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F722ICKX.build.board=GENERIC_F722ICKX
GenF7.menu.pnum.GENERIC_F722ICKX.build.product_line=STM32F722xx
GenF7.menu.pnum.GENERIC_F722ICKX.build.variant=STM32F7xx/F722I(C-E)(K-T)_F732IE(K-T)
GenF7.menu.pnum.GENERIC_F722ICKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F722.svd

# Generic F722IEKx
GenF7.menu.pnum.GENERIC_F722IEKX=Generic F722IEKx
GenF7.menu.pnum.GENERIC_F722IEKX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F722IEKX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F722IEKX.build.board=GENERIC_F722IEKX
GenF7.menu.pnum.GENERIC_F722IEKX.build.product_line=STM32F722xx
GenF7.menu.pnum.GENERIC_F722IEKX.build.variant=STM32F7xx/F722I(C-E)(K-T)_F732IE(K-T)
GenF7.menu.pnum.GENERIC_F722IEKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F722.svd

# Generic F722ICTx
GenF7.menu.pnum.GENERIC_F722ICTX=Generic F722ICTx
GenF7.menu.pnum.GENERIC_F722ICTX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F722ICTX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F722ICTX.build.board=GENERIC_F722ICTX
GenF7.menu.pnum.GENERIC_F722ICTX.build.product_line=STM32F722xx
GenF7.menu.pnum.GENERIC_F722ICTX.build.variant=STM32F7xx/F722I(C-E)(K-T)_F732IE(K-T)
GenF7.menu.pnum.GENERIC_F722ICTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F722.svd

# Generic F722IETx
GenF7.menu.pnum.GENERIC_F722IETX=Generic F722IETx
GenF7.menu.pnum.GENERIC_F722IETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F722IETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F722IETX.build.board=GENERIC_F722IETX
GenF7.menu.pnum.GENERIC_F722IETX.build.product_line=STM32F722xx
GenF7.menu.pnum.GENERIC_F722IETX.build.variant=STM32F7xx/F722I(C-E)(K-T)_F732IE(K-T)
GenF7.menu.pnum.GENERIC_F722IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F722.svd

# Generic F732IEKx
GenF7.menu.pnum.GENERIC_F732IEKX=Generic F732IEKx
GenF7.menu.pnum.GENERIC_F732IEKX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F732IEKX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F732IEKX.build.board=GENERIC_F732IEKX
GenF7.menu.pnum.GENERIC_F732IEKX.build.product_line=STM32F732xx
GenF7.menu.pnum.GENERIC_F732IEKX.build.variant=STM32F7xx/F722I(C-E)(K-T)_F732IE(K-T)
GenF7.menu.pnum.GENERIC_F732IEKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F732.svd

# Generic F732IETx
GenF7.menu.pnum.GENERIC_F732IETX=Generic F732IETx
GenF7.menu.pnum.GENERIC_F732IETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F732IETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F732IETX.build.board=GENERIC_F732IETX
GenF7.menu.pnum.GENERIC_F732IETX.build.product_line=STM32F732xx
GenF7.menu.pnum.GENERIC_F732IETX.build.variant=STM32F7xx/F722I(C-E)(K-T)_F732IE(K-T)
GenF7.menu.pnum.GENERIC_F732IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F732.svd

