# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F410R8Ix
GenF4.menu.pnum.GENERIC_F410R8IX=Generic F410R8Ix
GenF4.menu.pnum.GENERIC_F410R8IX.upload.maximum_size=65536
GenF4.menu.pnum.GENERIC_F410R8IX.upload.maximum_data_size=32768
GenF4.menu.pnum.GENERIC_F410R8IX.build.board=GENERIC_F410R8IX
GenF4.menu.pnum.GENERIC_F410R8IX.build.product_line=STM32F410Rx
GenF4.menu.pnum.GENERIC_F410R8IX.build.variant=STM32F4xx/F410R(8-B)(I-T)
GenF4.menu.pnum.GENERIC_F410R8IX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F410.svd

# Generic F410RBIx
GenF4.menu.pnum.GENERIC_F410RBIX=Generic F410RBIx
GenF4.menu.pnum.GENERIC_F410RBIX.upload.maximum_size=131072
GenF4.menu.pnum.GENERIC_F410RBIX.upload.maximum_data_size=32768
GenF4.menu.pnum.GENERIC_F410RBIX.build.board=GENERIC_F410RBIX
GenF4.menu.pnum.GENERIC_F410RBIX.build.product_line=STM32F410Rx
GenF4.menu.pnum.GENERIC_F410RBIX.build.variant=STM32F4xx/F410R(8-B)(I-T)
GenF4.menu.pnum.GENERIC_F410RBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F410.svd

# Generic F410R8Tx
GenF4.menu.pnum.GENERIC_F410R8TX=Generic F410R8Tx
GenF4.menu.pnum.GENERIC_F410R8TX.upload.maximum_size=65536
GenF4.menu.pnum.GENERIC_F410R8TX.upload.maximum_data_size=32768
GenF4.menu.pnum.GENERIC_F410R8TX.build.board=GENERIC_F410R8TX
GenF4.menu.pnum.GENERIC_F410R8TX.build.product_line=STM32F410Rx
GenF4.menu.pnum.GENERIC_F410R8TX.build.variant=STM32F4xx/F410R(8-B)(I-T)
GenF4.menu.pnum.GENERIC_F410R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F410.svd

# Generic F410RBTx
GenF4.menu.pnum.GENERIC_F410RBTX=Generic F410RBTx
GenF4.menu.pnum.GENERIC_F410RBTX.upload.maximum_size=131072
GenF4.menu.pnum.GENERIC_F410RBTX.upload.maximum_data_size=32768
GenF4.menu.pnum.GENERIC_F410RBTX.build.board=GENERIC_F410RBTX
GenF4.menu.pnum.GENERIC_F410RBTX.build.product_line=STM32F410Rx
GenF4.menu.pnum.GENERIC_F410RBTX.build.variant=STM32F4xx/F410R(8-B)(I-T)
GenF4.menu.pnum.GENERIC_F410RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F410.svd

