# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F768AIYx
GenF7.menu.pnum.GENERIC_F768AIYX=Generic F768AIYx
GenF7.menu.pnum.GENERIC_F768AIYX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F768AIYX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F768AIYX.build.board=GENERIC_F768AIYX
GenF7.menu.pnum.GENERIC_F768AIYX.build.product_line=STM32F769xx
GenF7.menu.pnum.GENERIC_F768AIYX.build.variant=STM32F7xx/F768AIY_F769A(G-I)Y_F778AIY_F779AIY
GenF7.menu.pnum.GENERIC_F768AIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F768.svd

# Generic F769AGYx
GenF7.menu.pnum.GENERIC_F769AGYX=Generic F769AGYx
GenF7.menu.pnum.GENERIC_F769AGYX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F769AGYX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F769AGYX.build.board=GENERIC_F769AGYX
GenF7.menu.pnum.GENERIC_F769AGYX.build.product_line=STM32F769xx
GenF7.menu.pnum.GENERIC_F769AGYX.build.variant=STM32F7xx/F768AIY_F769A(G-I)Y_F778AIY_F779AIY
GenF7.menu.pnum.GENERIC_F769AGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F769.svd

# Generic F769AIYx
GenF7.menu.pnum.GENERIC_F769AIYX=Generic F769AIYx
GenF7.menu.pnum.GENERIC_F769AIYX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F769AIYX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F769AIYX.build.board=GENERIC_F769AIYX
GenF7.menu.pnum.GENERIC_F769AIYX.build.product_line=STM32F769xx
GenF7.menu.pnum.GENERIC_F769AIYX.build.variant=STM32F7xx/F768AIY_F769A(G-I)Y_F778AIY_F779AIY
GenF7.menu.pnum.GENERIC_F769AIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F769.svd

# Generic F778AIYx
GenF7.menu.pnum.GENERIC_F778AIYX=Generic F778AIYx
GenF7.menu.pnum.GENERIC_F778AIYX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F778AIYX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F778AIYX.build.board=GENERIC_F778AIYX
GenF7.menu.pnum.GENERIC_F778AIYX.build.product_line=STM32F779xx
GenF7.menu.pnum.GENERIC_F778AIYX.build.variant=STM32F7xx/F768AIY_F769A(G-I)Y_F778AIY_F779AIY
GenF7.menu.pnum.GENERIC_F778AIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F778.svd

# Generic F779AIYx
GenF7.menu.pnum.GENERIC_F779AIYX=Generic F779AIYx
GenF7.menu.pnum.GENERIC_F779AIYX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F779AIYX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F779AIYX.build.board=GENERIC_F779AIYX
GenF7.menu.pnum.GENERIC_F779AIYX.build.product_line=STM32F779xx
GenF7.menu.pnum.GENERIC_F779AIYX.build.variant=STM32F7xx/F768AIY_F769A(G-I)Y_F778AIY_F779AIY
GenF7.menu.pnum.GENERIC_F779AIYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F779.svd

