# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G0B1CBTxN
GenG0.menu.pnum.GENERIC_G0B1CBTXN=Generic G0B1CBTxN
GenG0.menu.pnum.GENERIC_G0B1CBTXN.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G0B1CBTXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0B1CBTXN.build.board=GENERIC_G0B1CBTXN
GenG0.menu.pnum.GENERIC_G0B1CBTXN.build.product_line=STM32G0B1xx
GenG0.menu.pnum.GENERIC_G0B1CBTXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0B1CBTXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0B1.svd

# Generic G0B1CCTxN
GenG0.menu.pnum.GENERIC_G0B1CCTXN=Generic G0B1CCTxN
GenG0.menu.pnum.GENERIC_G0B1CCTXN.upload.maximum_size=262144
GenG0.menu.pnum.GENERIC_G0B1CCTXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0B1CCTXN.build.board=GENERIC_G0B1CCTXN
GenG0.menu.pnum.GENERIC_G0B1CCTXN.build.product_line=STM32G0B1xx
GenG0.menu.pnum.GENERIC_G0B1CCTXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0B1CCTXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0B1.svd

# Generic G0B1CETxN
GenG0.menu.pnum.GENERIC_G0B1CETXN=Generic G0B1CETxN
GenG0.menu.pnum.GENERIC_G0B1CETXN.upload.maximum_size=524288
GenG0.menu.pnum.GENERIC_G0B1CETXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0B1CETXN.build.board=GENERIC_G0B1CETXN
GenG0.menu.pnum.GENERIC_G0B1CETXN.build.product_line=STM32G0B1xx
GenG0.menu.pnum.GENERIC_G0B1CETXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0B1CETXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0B1.svd

# Generic G0B1CBUxN
GenG0.menu.pnum.GENERIC_G0B1CBUXN=Generic G0B1CBUxN
GenG0.menu.pnum.GENERIC_G0B1CBUXN.upload.maximum_size=131072
GenG0.menu.pnum.GENERIC_G0B1CBUXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0B1CBUXN.build.board=GENERIC_G0B1CBUXN
GenG0.menu.pnum.GENERIC_G0B1CBUXN.build.product_line=STM32G0B1xx
GenG0.menu.pnum.GENERIC_G0B1CBUXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0B1CBUXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0B1.svd

# Generic G0B1CCUxN
GenG0.menu.pnum.GENERIC_G0B1CCUXN=Generic G0B1CCUxN
GenG0.menu.pnum.GENERIC_G0B1CCUXN.upload.maximum_size=262144
GenG0.menu.pnum.GENERIC_G0B1CCUXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0B1CCUXN.build.board=GENERIC_G0B1CCUXN
GenG0.menu.pnum.GENERIC_G0B1CCUXN.build.product_line=STM32G0B1xx
GenG0.menu.pnum.GENERIC_G0B1CCUXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0B1CCUXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0B1.svd

# Generic G0B1CEUxN
GenG0.menu.pnum.GENERIC_G0B1CEUXN=Generic G0B1CEUxN
GenG0.menu.pnum.GENERIC_G0B1CEUXN.upload.maximum_size=524288
GenG0.menu.pnum.GENERIC_G0B1CEUXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0B1CEUXN.build.board=GENERIC_G0B1CEUXN
GenG0.menu.pnum.GENERIC_G0B1CEUXN.build.product_line=STM32G0B1xx
GenG0.menu.pnum.GENERIC_G0B1CEUXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0B1CEUXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0B1.svd

# Generic G0C1CCTxN
GenG0.menu.pnum.GENERIC_G0C1CCTXN=Generic G0C1CCTxN
GenG0.menu.pnum.GENERIC_G0C1CCTXN.upload.maximum_size=262144
GenG0.menu.pnum.GENERIC_G0C1CCTXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0C1CCTXN.build.board=GENERIC_G0C1CCTXN
GenG0.menu.pnum.GENERIC_G0C1CCTXN.build.product_line=STM32G0C1xx
GenG0.menu.pnum.GENERIC_G0C1CCTXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0C1CCTXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0C1.svd

# Generic G0C1CETxN
GenG0.menu.pnum.GENERIC_G0C1CETXN=Generic G0C1CETxN
GenG0.menu.pnum.GENERIC_G0C1CETXN.upload.maximum_size=524288
GenG0.menu.pnum.GENERIC_G0C1CETXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0C1CETXN.build.board=GENERIC_G0C1CETXN
GenG0.menu.pnum.GENERIC_G0C1CETXN.build.product_line=STM32G0C1xx
GenG0.menu.pnum.GENERIC_G0C1CETXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0C1CETXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0C1.svd

# Generic G0C1CCUxN
GenG0.menu.pnum.GENERIC_G0C1CCUXN=Generic G0C1CCUxN
GenG0.menu.pnum.GENERIC_G0C1CCUXN.upload.maximum_size=262144
GenG0.menu.pnum.GENERIC_G0C1CCUXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0C1CCUXN.build.board=GENERIC_G0C1CCUXN
GenG0.menu.pnum.GENERIC_G0C1CCUXN.build.product_line=STM32G0C1xx
GenG0.menu.pnum.GENERIC_G0C1CCUXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0C1CCUXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0C1.svd

# Generic G0C1CEUxN
GenG0.menu.pnum.GENERIC_G0C1CEUXN=Generic G0C1CEUxN
GenG0.menu.pnum.GENERIC_G0C1CEUXN.upload.maximum_size=524288
GenG0.menu.pnum.GENERIC_G0C1CEUXN.upload.maximum_data_size=147456
GenG0.menu.pnum.GENERIC_G0C1CEUXN.build.board=GENERIC_G0C1CEUXN
GenG0.menu.pnum.GENERIC_G0C1CEUXN.build.product_line=STM32G0C1xx
GenG0.menu.pnum.GENERIC_G0C1CEUXN.build.variant=STM32G0xx/G0B1C(B-C-E)(T-U)xN_G0C1C(C-E)(T-U)xN
GenG0.menu.pnum.GENERIC_G0C1CEUXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G0C1.svd

