# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L010K4Tx
GenL0.menu.pnum.GENERIC_L010K4TX=Generic L010K4Tx
GenL0.menu.pnum.GENERIC_L010K4TX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L010K4TX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L010K4TX.build.board=GENERIC_L010K4TX
GenL0.menu.pnum.GENERIC_L010K4TX.build.product_line=STM32L010x4
GenL0.menu.pnum.GENERIC_L010K4TX.build.variant=STM32L0xx/L010K4T_L011K(3-4)T_L021K4T
GenL0.menu.pnum.GENERIC_L010K4TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x0.svd

# Generic L011K3Tx
GenL0.menu.pnum.GENERIC_L011K3TX=Generic L011K3Tx
GenL0.menu.pnum.GENERIC_L011K3TX.upload.maximum_size=8192
GenL0.menu.pnum.GENERIC_L011K3TX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011K3TX.build.board=GENERIC_L011K3TX
GenL0.menu.pnum.GENERIC_L011K3TX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011K3TX.build.variant=STM32L0xx/L010K4T_L011K(3-4)T_L021K4T
GenL0.menu.pnum.GENERIC_L011K3TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L011K4Tx
GenL0.menu.pnum.GENERIC_L011K4TX=Generic L011K4Tx
GenL0.menu.pnum.GENERIC_L011K4TX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L011K4TX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L011K4TX.build.board=GENERIC_L011K4TX
GenL0.menu.pnum.GENERIC_L011K4TX.build.product_line=STM32L011xx
GenL0.menu.pnum.GENERIC_L011K4TX.build.variant=STM32L0xx/L010K4T_L011K(3-4)T_L021K4T
GenL0.menu.pnum.GENERIC_L011K4TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L021K4Tx
GenL0.menu.pnum.GENERIC_L021K4TX=Generic L021K4Tx
GenL0.menu.pnum.GENERIC_L021K4TX.upload.maximum_size=16384
GenL0.menu.pnum.GENERIC_L021K4TX.upload.maximum_data_size=2048
GenL0.menu.pnum.GENERIC_L021K4TX.build.board=GENERIC_L021K4TX
GenL0.menu.pnum.GENERIC_L021K4TX.build.product_line=STM32L021xx
GenL0.menu.pnum.GENERIC_L021K4TX.build.variant=STM32L0xx/L010K4T_L011K(3-4)T_L021K4T
GenL0.menu.pnum.GENERIC_L021K4TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

