# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G051G6Ux
GenG0.menu.pnum.GENERIC_G051G6UX=Generic G051G6Ux
GenG0.menu.pnum.GENERIC_G051G6UX.upload.maximum_size=32768
GenG0.menu.pnum.GENERIC_G051G6UX.upload.maximum_data_size=18432
GenG0.menu.pnum.GENERIC_G051G6UX.build.board=GENERIC_G051G6UX
GenG0.menu.pnum.GENERIC_G051G6UX.build.product_line=STM32G051xx
GenG0.menu.pnum.GENERIC_G051G6UX.build.variant=STM32G0xx/G051G(6-8)U_G061G(6-8)U
GenG0.menu.pnum.GENERIC_G051G6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G051.svd

# Generic G051G8Ux
GenG0.menu.pnum.GENERIC_G051G8UX=Generic G051G8Ux
GenG0.menu.pnum.GENERIC_G051G8UX.upload.maximum_size=65536
GenG0.menu.pnum.GENERIC_G051G8UX.upload.maximum_data_size=18432
GenG0.menu.pnum.GENERIC_G051G8UX.build.board=GENERIC_G051G8UX
GenG0.menu.pnum.GENERIC_G051G8UX.build.product_line=STM32G051xx
GenG0.menu.pnum.GENERIC_G051G8UX.build.variant=STM32G0xx/G051G(6-8)U_G061G(6-8)U
GenG0.menu.pnum.GENERIC_G051G8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G051.svd

# Generic G061G6Ux
GenG0.menu.pnum.GENERIC_G061G6UX=Generic G061G6Ux
GenG0.menu.pnum.GENERIC_G061G6UX.upload.maximum_size=32768
GenG0.menu.pnum.GENERIC_G061G6UX.upload.maximum_data_size=18432
GenG0.menu.pnum.GENERIC_G061G6UX.build.board=GENERIC_G061G6UX
GenG0.menu.pnum.GENERIC_G061G6UX.build.product_line=STM32G061xx
GenG0.menu.pnum.GENERIC_G061G6UX.build.variant=STM32G0xx/G051G(6-8)U_G061G(6-8)U
GenG0.menu.pnum.GENERIC_G061G6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G061.svd

# Generic G061G8Ux
GenG0.menu.pnum.GENERIC_G061G8UX=Generic G061G8Ux
GenG0.menu.pnum.GENERIC_G061G8UX.upload.maximum_size=65536
GenG0.menu.pnum.GENERIC_G061G8UX.upload.maximum_data_size=18432
GenG0.menu.pnum.GENERIC_G061G8UX.build.board=GENERIC_G061G8UX
GenG0.menu.pnum.GENERIC_G061G8UX.build.product_line=STM32G061xx
GenG0.menu.pnum.GENERIC_G061G8UX.build.variant=STM32G0xx/G051G(6-8)U_G061G(6-8)U
GenG0.menu.pnum.GENERIC_G061G8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G0xx/STM32G061.svd

