# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F071V8Hx
GenF0.menu.pnum.GENERIC_F071V8HX=Generic F071V8Hx
GenF0.menu.pnum.GENERIC_F071V8HX.upload.maximum_size=65536
GenF0.menu.pnum.GENERIC_F071V8HX.upload.maximum_data_size=16384
GenF0.menu.pnum.GENERIC_F071V8HX.build.board=GENERIC_F071V8HX
GenF0.menu.pnum.GENERIC_F071V8HX.build.product_line=STM32F071xB
GenF0.menu.pnum.GENERIC_F071V8HX.build.variant=STM32F0xx/F071V(8-B)(H-T)
GenF0.menu.pnum.GENERIC_F071V8HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F071VBHx
GenF0.menu.pnum.GENERIC_F071VBHX=Generic F071VBHx
GenF0.menu.pnum.GENERIC_F071VBHX.upload.maximum_size=131072
GenF0.menu.pnum.GENERIC_F071VBHX.upload.maximum_data_size=16384
GenF0.menu.pnum.GENERIC_F071VBHX.build.board=GENERIC_F071VBHX
GenF0.menu.pnum.GENERIC_F071VBHX.build.product_line=STM32F071xB
GenF0.menu.pnum.GENERIC_F071VBHX.build.variant=STM32F0xx/F071V(8-B)(H-T)
GenF0.menu.pnum.GENERIC_F071VBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F071V8Tx
GenF0.menu.pnum.GENERIC_F071V8TX=Generic F071V8Tx
GenF0.menu.pnum.GENERIC_F071V8TX.upload.maximum_size=65536
GenF0.menu.pnum.GENERIC_F071V8TX.upload.maximum_data_size=16384
GenF0.menu.pnum.GENERIC_F071V8TX.build.board=GENERIC_F071V8TX
GenF0.menu.pnum.GENERIC_F071V8TX.build.product_line=STM32F071xB
GenF0.menu.pnum.GENERIC_F071V8TX.build.variant=STM32F0xx/F071V(8-B)(H-T)
GenF0.menu.pnum.GENERIC_F071V8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

# Generic F071VBTx
GenF0.menu.pnum.GENERIC_F071VBTX=Generic F071VBTx
GenF0.menu.pnum.GENERIC_F071VBTX.upload.maximum_size=131072
GenF0.menu.pnum.GENERIC_F071VBTX.upload.maximum_data_size=16384
GenF0.menu.pnum.GENERIC_F071VBTX.build.board=GENERIC_F071VBTX
GenF0.menu.pnum.GENERIC_F071VBTX.build.product_line=STM32F071xB
GenF0.menu.pnum.GENERIC_F071VBTX.build.variant=STM32F0xx/F071V(8-B)(H-T)
GenF0.menu.pnum.GENERIC_F071VBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F0xx/STM32F0x1.svd

