# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F765ZGTx
GenF7.menu.pnum.GENERIC_F765ZGTX=Generic F765ZGTx
GenF7.menu.pnum.GENERIC_F765ZGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F765ZGTX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F765ZGTX.build.board=GENERIC_F765ZGTX
GenF7.menu.pnum.GENERIC_F765ZGTX.build.product_line=STM32F765xx
GenF7.menu.pnum.GENERIC_F765ZGTX.build.variant=STM32F7xx/F765Z(G-I)T_F767Z(G-I)T_F777ZIT
GenF7.menu.pnum.GENERIC_F765ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F765.svd

# Generic F765ZITx
GenF7.menu.pnum.GENERIC_F765ZITX=Generic F765ZITx
GenF7.menu.pnum.GENERIC_F765ZITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F765ZITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F765ZITX.build.board=GENERIC_F765ZITX
GenF7.menu.pnum.GENERIC_F765ZITX.build.product_line=STM32F765xx
GenF7.menu.pnum.GENERIC_F765ZITX.build.variant=STM32F7xx/F765Z(G-I)T_F767Z(G-I)T_F777ZIT
GenF7.menu.pnum.GENERIC_F765ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F765.svd

# Generic F767ZGTx
GenF7.menu.pnum.GENERIC_F767ZGTX=Generic F767ZGTx
GenF7.menu.pnum.GENERIC_F767ZGTX.upload.maximum_size=1048576
GenF7.menu.pnum.GENERIC_F767ZGTX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F767ZGTX.build.board=GENERIC_F767ZGTX
GenF7.menu.pnum.GENERIC_F767ZGTX.build.product_line=STM32F767xx
GenF7.menu.pnum.GENERIC_F767ZGTX.build.variant=STM32F7xx/F765Z(G-I)T_F767Z(G-I)T_F777ZIT
GenF7.menu.pnum.GENERIC_F767ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F767.svd

# Generic F767ZITx
GenF7.menu.pnum.GENERIC_F767ZITX=Generic F767ZITx
GenF7.menu.pnum.GENERIC_F767ZITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F767ZITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F767ZITX.build.board=GENERIC_F767ZITX
GenF7.menu.pnum.GENERIC_F767ZITX.build.product_line=STM32F767xx
GenF7.menu.pnum.GENERIC_F767ZITX.build.variant=STM32F7xx/F765Z(G-I)T_F767Z(G-I)T_F777ZIT
GenF7.menu.pnum.GENERIC_F767ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F767.svd

# Generic F777ZITx
GenF7.menu.pnum.GENERIC_F777ZITX=Generic F777ZITx
GenF7.menu.pnum.GENERIC_F777ZITX.upload.maximum_size=2097152
GenF7.menu.pnum.GENERIC_F777ZITX.upload.maximum_data_size=393216
GenF7.menu.pnum.GENERIC_F777ZITX.build.board=GENERIC_F777ZITX
GenF7.menu.pnum.GENERIC_F777ZITX.build.product_line=STM32F777xx
GenF7.menu.pnum.GENERIC_F777ZITX.build.variant=STM32F7xx/F765Z(G-I)T_F767Z(G-I)T_F777ZIT
GenF7.menu.pnum.GENERIC_F777ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F777.svd

