# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L433CBTx
GenL4.menu.pnum.GENERIC_L433CBTX=Generic L433CBTx
GenL4.menu.pnum.GENERIC_L433CBTX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L433CBTX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433CBTX.build.board=GENERIC_L433CBTX
GenL4.menu.pnum.GENERIC_L433CBTX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433CBTX.build.variant=STM32L4xx/L433C(B-C)(T-U)_L443CC(T-U)
GenL4.menu.pnum.GENERIC_L433CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L433CCTx
GenL4.menu.pnum.GENERIC_L433CCTX=Generic L433CCTx
GenL4.menu.pnum.GENERIC_L433CCTX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L433CCTX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433CCTX.build.board=GENERIC_L433CCTX
GenL4.menu.pnum.GENERIC_L433CCTX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433CCTX.build.variant=STM32L4xx/L433C(B-C)(T-U)_L443CC(T-U)
GenL4.menu.pnum.GENERIC_L433CCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L433CBUx
GenL4.menu.pnum.GENERIC_L433CBUX=Generic L433CBUx
GenL4.menu.pnum.GENERIC_L433CBUX.upload.maximum_size=131072
GenL4.menu.pnum.GENERIC_L433CBUX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433CBUX.build.board=GENERIC_L433CBUX
GenL4.menu.pnum.GENERIC_L433CBUX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433CBUX.build.variant=STM32L4xx/L433C(B-C)(T-U)_L443CC(T-U)
GenL4.menu.pnum.GENERIC_L433CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L433CCUx
GenL4.menu.pnum.GENERIC_L433CCUX=Generic L433CCUx
GenL4.menu.pnum.GENERIC_L433CCUX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L433CCUX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433CCUX.build.board=GENERIC_L433CCUX
GenL4.menu.pnum.GENERIC_L433CCUX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433CCUX.build.variant=STM32L4xx/L433C(B-C)(T-U)_L443CC(T-U)
GenL4.menu.pnum.GENERIC_L433CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L443CCTx
GenL4.menu.pnum.GENERIC_L443CCTX=Generic L443CCTx
GenL4.menu.pnum.GENERIC_L443CCTX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L443CCTX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L443CCTX.build.board=GENERIC_L443CCTX
GenL4.menu.pnum.GENERIC_L443CCTX.build.product_line=STM32L443xx
GenL4.menu.pnum.GENERIC_L443CCTX.build.variant=STM32L4xx/L433C(B-C)(T-U)_L443CC(T-U)
GenL4.menu.pnum.GENERIC_L443CCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L443.svd

# Generic L443CCUx
GenL4.menu.pnum.GENERIC_L443CCUX=Generic L443CCUx
GenL4.menu.pnum.GENERIC_L443CCUX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L443CCUX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L443CCUX.build.board=GENERIC_L443CCUX
GenL4.menu.pnum.GENERIC_L443CCUX.build.product_line=STM32L443xx
GenL4.menu.pnum.GENERIC_L443CCUX.build.variant=STM32L4xx/L433C(B-C)(T-U)_L443CC(T-U)
GenL4.menu.pnum.GENERIC_L443CCUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L443.svd

