# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F105R8Tx
GenF1.menu.pnum.GENERIC_F105R8TX=Generic F105R8Tx
GenF1.menu.pnum.GENERIC_F105R8TX.upload.maximum_size=65536
GenF1.menu.pnum.GENERIC_F105R8TX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105R8TX.build.board=GENERIC_F105R8TX
GenF1.menu.pnum.GENERIC_F105R8TX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105R8TX.build.variant=STM32F1xx/F105R(8-B-C)T
GenF1.menu.pnum.GENERIC_F105R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

# Generic F105RBTx
GenF1.menu.pnum.GENERIC_F105RBTX=Generic F105RBTx
GenF1.menu.pnum.GENERIC_F105RBTX.upload.maximum_size=131072
GenF1.menu.pnum.GENERIC_F105RBTX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105RBTX.build.board=GENERIC_F105RBTX
GenF1.menu.pnum.GENERIC_F105RBTX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105RBTX.build.variant=STM32F1xx/F105R(8-B-C)T
GenF1.menu.pnum.GENERIC_F105RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

# Generic F105RCTx
GenF1.menu.pnum.GENERIC_F105RCTX=Generic F105RCTx
GenF1.menu.pnum.GENERIC_F105RCTX.upload.maximum_size=262144
GenF1.menu.pnum.GENERIC_F105RCTX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F105RCTX.build.board=GENERIC_F105RCTX
GenF1.menu.pnum.GENERIC_F105RCTX.build.product_line=STM32F105xC
GenF1.menu.pnum.GENERIC_F105RCTX.build.variant=STM32F1xx/F105R(8-B-C)T
GenF1.menu.pnum.GENERIC_F105RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F105.svd

