# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic H563AIIxQ
GenH5.menu.pnum.GENERIC_H563AIIXQ=Generic H563AIIxQ
GenH5.menu.pnum.GENERIC_H563AIIXQ.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H563AIIXQ.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H563AIIXQ.build.board=GENERIC_H563AIIXQ
GenH5.menu.pnum.GENERIC_H563AIIXQ.build.product_line=STM32H563xx
GenH5.menu.pnum.GENERIC_H563AIIXQ.build.variant=STM32H5xx/H563AIIxQ_H573AIIxQ
GenH5.menu.pnum.GENERIC_H563AIIXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H563.svd

# Generic H573AIIxQ
GenH5.menu.pnum.GENERIC_H573AIIXQ=Generic H573AIIxQ
GenH5.menu.pnum.GENERIC_H573AIIXQ.upload.maximum_size=2097152
GenH5.menu.pnum.GENERIC_H573AIIXQ.upload.maximum_data_size=655360
GenH5.menu.pnum.GENERIC_H573AIIXQ.build.board=GENERIC_H573AIIXQ
GenH5.menu.pnum.GENERIC_H573AIIXQ.build.product_line=STM32H573xx
GenH5.menu.pnum.GENERIC_H573AIIXQ.build.variant=STM32H5xx/H563AIIxQ_H573AIIxQ
GenH5.menu.pnum.GENERIC_H573AIIXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H573.svd

