# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G431M6Tx
GenG4.menu.pnum.GENERIC_G431M6TX=Generic G431M6Tx
GenG4.menu.pnum.GENERIC_G431M6TX.upload.maximum_size=32768
GenG4.menu.pnum.GENERIC_G431M6TX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431M6TX.build.board=GENERIC_G431M6TX
GenG4.menu.pnum.GENERIC_G431M6TX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431M6TX.build.variant=STM32G4xx/G431M(6-8-B)T_G441MBT
GenG4.menu.pnum.GENERIC_G431M6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G431M8Tx
GenG4.menu.pnum.GENERIC_G431M8TX=Generic G431M8Tx
GenG4.menu.pnum.GENERIC_G431M8TX.upload.maximum_size=65536
GenG4.menu.pnum.GENERIC_G431M8TX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431M8TX.build.board=GENERIC_G431M8TX
GenG4.menu.pnum.GENERIC_G431M8TX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431M8TX.build.variant=STM32G4xx/G431M(6-8-B)T_G441MBT
GenG4.menu.pnum.GENERIC_G431M8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G431MBTx
GenG4.menu.pnum.GENERIC_G431MBTX=Generic G431MBTx
GenG4.menu.pnum.GENERIC_G431MBTX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G431MBTX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G431MBTX.build.board=GENERIC_G431MBTX
GenG4.menu.pnum.GENERIC_G431MBTX.build.product_line=STM32G431xx
GenG4.menu.pnum.GENERIC_G431MBTX.build.variant=STM32G4xx/G431M(6-8-B)T_G441MBT
GenG4.menu.pnum.GENERIC_G431MBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G431.svd

# Generic G441MBTx
GenG4.menu.pnum.GENERIC_G441MBTX=Generic G441MBTx
GenG4.menu.pnum.GENERIC_G441MBTX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G441MBTX.upload.maximum_data_size=32768
GenG4.menu.pnum.GENERIC_G441MBTX.build.board=GENERIC_G441MBTX
GenG4.menu.pnum.GENERIC_G441MBTX.build.product_line=STM32G441xx
GenG4.menu.pnum.GENERIC_G441MBTX.build.variant=STM32G4xx/G431M(6-8-B)T_G441MBT
GenG4.menu.pnum.GENERIC_G441MBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G441.svd

