# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L071CBTx
GenL0.menu.pnum.GENERIC_L071CBTX=Generic L071CBTx
GenL0.menu.pnum.GENERIC_L071CBTX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L071CBTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071CBTX.build.board=GENERIC_L071CBTX
GenL0.menu.pnum.GENERIC_L071CBTX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071CBTX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L071CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071CZTx
GenL0.menu.pnum.GENERIC_L071CZTX=Generic L071CZTx
GenL0.menu.pnum.GENERIC_L071CZTX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L071CZTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071CZTX.build.board=GENERIC_L071CZTX
GenL0.menu.pnum.GENERIC_L071CZTX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071CZTX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L071CZTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071CBUx
GenL0.menu.pnum.GENERIC_L071CBUX=Generic L071CBUx
GenL0.menu.pnum.GENERIC_L071CBUX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L071CBUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071CBUX.build.board=GENERIC_L071CBUX
GenL0.menu.pnum.GENERIC_L071CBUX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071CBUX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L071CBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071CZUx
GenL0.menu.pnum.GENERIC_L071CZUX=Generic L071CZUx
GenL0.menu.pnum.GENERIC_L071CZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L071CZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071CZUX.build.board=GENERIC_L071CZUX
GenL0.menu.pnum.GENERIC_L071CZUX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071CZUX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L071CZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071C8Tx
GenL0.menu.pnum.GENERIC_L071C8TX=Generic L071C8Tx
GenL0.menu.pnum.GENERIC_L071C8TX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L071C8TX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071C8TX.build.board=GENERIC_L071C8TX
GenL0.menu.pnum.GENERIC_L071C8TX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071C8TX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L071C8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071C8Ux
GenL0.menu.pnum.GENERIC_L071C8UX=Generic L071C8Ux
GenL0.menu.pnum.GENERIC_L071C8UX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L071C8UX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071C8UX.build.board=GENERIC_L071C8UX
GenL0.menu.pnum.GENERIC_L071C8UX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071C8UX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L071C8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L081CBTx
GenL0.menu.pnum.GENERIC_L081CBTX=Generic L081CBTx
GenL0.menu.pnum.GENERIC_L081CBTX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L081CBTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L081CBTX.build.board=GENERIC_L081CBTX
GenL0.menu.pnum.GENERIC_L081CBTX.build.product_line=STM32L081xx
GenL0.menu.pnum.GENERIC_L081CBTX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L081CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L081CZTx
GenL0.menu.pnum.GENERIC_L081CZTX=Generic L081CZTx
GenL0.menu.pnum.GENERIC_L081CZTX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L081CZTX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L081CZTX.build.board=GENERIC_L081CZTX
GenL0.menu.pnum.GENERIC_L081CZTX.build.product_line=STM32L081xx
GenL0.menu.pnum.GENERIC_L081CZTX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L081CZTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L081CZUx
GenL0.menu.pnum.GENERIC_L081CZUX=Generic L081CZUx
GenL0.menu.pnum.GENERIC_L081CZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L081CZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L081CZUX.build.board=GENERIC_L081CZUX
GenL0.menu.pnum.GENERIC_L081CZUX.build.product_line=STM32L081xx
GenL0.menu.pnum.GENERIC_L081CZUX.build.variant=STM32L0xx/L071C(8-B-Z)(T-U)_L081CBT_L081CZ(T-U)
GenL0.menu.pnum.GENERIC_L081CZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

