# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F722ZCTx
GenF7.menu.pnum.GENERIC_F722ZCTX=Generic F722ZCTx
GenF7.menu.pnum.GENERIC_F722ZCTX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F722ZCTX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F722ZCTX.build.board=GENERIC_F722ZCTX
GenF7.menu.pnum.GENERIC_F722ZCTX.build.product_line=STM32F722xx
GenF7.menu.pnum.GENERIC_F722ZCTX.build.variant=STM32F7xx/F722Z(C-E)T_F732ZET
GenF7.menu.pnum.GENERIC_F722ZCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F722.svd

# Generic F722ZETx
GenF7.menu.pnum.GENERIC_F722ZETX=Generic F722ZETx
GenF7.menu.pnum.GENERIC_F722ZETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F722ZETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F722ZETX.build.board=GENERIC_F722ZETX
GenF7.menu.pnum.GENERIC_F722ZETX.build.product_line=STM32F722xx
GenF7.menu.pnum.GENERIC_F722ZETX.build.variant=STM32F7xx/F722Z(C-E)T_F732ZET
GenF7.menu.pnum.GENERIC_F722ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F722.svd

# Generic F732ZETx
GenF7.menu.pnum.GENERIC_F732ZETX=Generic F732ZETx
GenF7.menu.pnum.GENERIC_F732ZETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F732ZETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F732ZETX.build.board=GENERIC_F732ZETX
GenF7.menu.pnum.GENERIC_F732ZETX.build.product_line=STM32F732xx
GenF7.menu.pnum.GENERIC_F732ZETX.build.variant=STM32F7xx/F722Z(C-E)T_F732ZET
GenF7.menu.pnum.GENERIC_F732ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F732.svd

