# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F446ZCHx
GenF4.menu.pnum.GENERIC_F446ZCHX=Generic F446ZCHx
GenF4.menu.pnum.GENERIC_F446ZCHX.upload.maximum_size=262144
GenF4.menu.pnum.GENERIC_F446ZCHX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F446ZCHX.build.board=GENERIC_F446ZCHX
GenF4.menu.pnum.GENERIC_F446ZCHX.build.product_line=STM32F446xx
GenF4.menu.pnum.GENERIC_F446ZCHX.build.variant=STM32F4xx/F446Z(C-E)(H-J-T)
GenF4.menu.pnum.GENERIC_F446ZCHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F446.svd

# Generic F446ZEHx
GenF4.menu.pnum.GENERIC_F446ZEHX=Generic F446ZEHx
GenF4.menu.pnum.GENERIC_F446ZEHX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F446ZEHX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F446ZEHX.build.board=GENERIC_F446ZEHX
GenF4.menu.pnum.GENERIC_F446ZEHX.build.product_line=STM32F446xx
GenF4.menu.pnum.GENERIC_F446ZEHX.build.variant=STM32F4xx/F446Z(C-E)(H-J-T)
GenF4.menu.pnum.GENERIC_F446ZEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F446.svd

# Generic F446ZCJx
GenF4.menu.pnum.GENERIC_F446ZCJX=Generic F446ZCJx
GenF4.menu.pnum.GENERIC_F446ZCJX.upload.maximum_size=262144
GenF4.menu.pnum.GENERIC_F446ZCJX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F446ZCJX.build.board=GENERIC_F446ZCJX
GenF4.menu.pnum.GENERIC_F446ZCJX.build.product_line=STM32F446xx
GenF4.menu.pnum.GENERIC_F446ZCJX.build.variant=STM32F4xx/F446Z(C-E)(H-J-T)
GenF4.menu.pnum.GENERIC_F446ZCJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F446.svd

# Generic F446ZEJx
GenF4.menu.pnum.GENERIC_F446ZEJX=Generic F446ZEJx
GenF4.menu.pnum.GENERIC_F446ZEJX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F446ZEJX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F446ZEJX.build.board=GENERIC_F446ZEJX
GenF4.menu.pnum.GENERIC_F446ZEJX.build.product_line=STM32F446xx
GenF4.menu.pnum.GENERIC_F446ZEJX.build.variant=STM32F4xx/F446Z(C-E)(H-J-T)
GenF4.menu.pnum.GENERIC_F446ZEJX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F446.svd

# Generic F446ZCTx
GenF4.menu.pnum.GENERIC_F446ZCTX=Generic F446ZCTx
GenF4.menu.pnum.GENERIC_F446ZCTX.upload.maximum_size=262144
GenF4.menu.pnum.GENERIC_F446ZCTX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F446ZCTX.build.board=GENERIC_F446ZCTX
GenF4.menu.pnum.GENERIC_F446ZCTX.build.product_line=STM32F446xx
GenF4.menu.pnum.GENERIC_F446ZCTX.build.variant=STM32F4xx/F446Z(C-E)(H-J-T)
GenF4.menu.pnum.GENERIC_F446ZCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F446.svd

# Generic F446ZETx
GenF4.menu.pnum.GENERIC_F446ZETX=Generic F446ZETx
GenF4.menu.pnum.GENERIC_F446ZETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F446ZETX.upload.maximum_data_size=131072
GenF4.menu.pnum.GENERIC_F446ZETX.build.board=GENERIC_F446ZETX
GenF4.menu.pnum.GENERIC_F446ZETX.build.product_line=STM32F446xx
GenF4.menu.pnum.GENERIC_F446ZETX.build.variant=STM32F4xx/F446Z(C-E)(H-J-T)
GenF4.menu.pnum.GENERIC_F446ZETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F446.svd

