# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F413CGUx
GenF4.menu.pnum.GENERIC_F413CGUX=Generic F413CGUx
GenF4.menu.pnum.GENERIC_F413CGUX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F413CGUX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F413CGUX.build.board=GENERIC_F413CGUX
GenF4.menu.pnum.GENERIC_F413CGUX.build.product_line=STM32F413xx
GenF4.menu.pnum.GENERIC_F413CGUX.build.variant=STM32F4xx/F413C(G-H)U_F423CHU
GenF4.menu.pnum.GENERIC_F413CGUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F413.svd

# Generic F413CHUx
GenF4.menu.pnum.GENERIC_F413CHUX=Generic F413CHUx
GenF4.menu.pnum.GENERIC_F413CHUX.upload.maximum_size=1572864
GenF4.menu.pnum.GENERIC_F413CHUX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F413CHUX.build.board=GENERIC_F413CHUX
GenF4.menu.pnum.GENERIC_F413CHUX.build.product_line=STM32F413xx
GenF4.menu.pnum.GENERIC_F413CHUX.build.variant=STM32F4xx/F413C(G-H)U_F423CHU
GenF4.menu.pnum.GENERIC_F413CHUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F413.svd

# Generic F423CHUx
GenF4.menu.pnum.GENERIC_F423CHUX=Generic F423CHUx
GenF4.menu.pnum.GENERIC_F423CHUX.upload.maximum_size=1572864
GenF4.menu.pnum.GENERIC_F423CHUX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F423CHUX.build.board=GENERIC_F423CHUX
GenF4.menu.pnum.GENERIC_F423CHUX.build.product_line=STM32F423xx
GenF4.menu.pnum.GENERIC_F423CHUX.build.variant=STM32F4xx/F413C(G-H)U_F423CHU
GenF4.menu.pnum.GENERIC_F423CHUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F423.svd

