# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F469IETx
GenF4.menu.pnum.GENERIC_F469IETX=Generic F469IETx
GenF4.menu.pnum.GENERIC_F469IETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F469IETX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469IETX.build.board=GENERIC_F469IETX
GenF4.menu.pnum.GENERIC_F469IETX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469IETX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F469IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469IGTx
GenF4.menu.pnum.GENERIC_F469IGTX=Generic F469IGTx
GenF4.menu.pnum.GENERIC_F469IGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F469IGTX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469IGTX.build.board=GENERIC_F469IGTX
GenF4.menu.pnum.GENERIC_F469IGTX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469IGTX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F469IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469IEHx
GenF4.menu.pnum.GENERIC_F469IEHX=Generic F469IEHx
GenF4.menu.pnum.GENERIC_F469IEHX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F469IEHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469IEHX.build.board=GENERIC_F469IEHX
GenF4.menu.pnum.GENERIC_F469IEHX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469IEHX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F469IEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469IGHx
GenF4.menu.pnum.GENERIC_F469IGHX=Generic F469IGHx
GenF4.menu.pnum.GENERIC_F469IGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F469IGHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469IGHX.build.board=GENERIC_F469IGHX
GenF4.menu.pnum.GENERIC_F469IGHX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469IGHX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F469IGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469IIHx
GenF4.menu.pnum.GENERIC_F469IIHX=Generic F469IIHx
GenF4.menu.pnum.GENERIC_F469IIHX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F469IIHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469IIHX.build.board=GENERIC_F469IIHX
GenF4.menu.pnum.GENERIC_F469IIHX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469IIHX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F469IIHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F469IITx
GenF4.menu.pnum.GENERIC_F469IITX=Generic F469IITx
GenF4.menu.pnum.GENERIC_F469IITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F469IITX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F469IITX.build.board=GENERIC_F469IITX
GenF4.menu.pnum.GENERIC_F469IITX.build.product_line=STM32F469xx
GenF4.menu.pnum.GENERIC_F469IITX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F469IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F469.svd

# Generic F479IGHx
GenF4.menu.pnum.GENERIC_F479IGHX=Generic F479IGHx
GenF4.menu.pnum.GENERIC_F479IGHX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F479IGHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479IGHX.build.board=GENERIC_F479IGHX
GenF4.menu.pnum.GENERIC_F479IGHX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479IGHX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F479IGHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

# Generic F479IIHx
GenF4.menu.pnum.GENERIC_F479IIHX=Generic F479IIHx
GenF4.menu.pnum.GENERIC_F479IIHX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F479IIHX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479IIHX.build.board=GENERIC_F479IIHX
GenF4.menu.pnum.GENERIC_F479IIHX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479IIHX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F479IIHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

# Generic F479IGTx
GenF4.menu.pnum.GENERIC_F479IGTX=Generic F479IGTx
GenF4.menu.pnum.GENERIC_F479IGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F479IGTX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479IGTX.build.board=GENERIC_F479IGTX
GenF4.menu.pnum.GENERIC_F479IGTX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479IGTX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F479IGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

# Generic F479IITx
GenF4.menu.pnum.GENERIC_F479IITX=Generic F479IITx
GenF4.menu.pnum.GENERIC_F479IITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F479IITX.upload.maximum_data_size=327680
GenF4.menu.pnum.GENERIC_F479IITX.build.board=GENERIC_F479IITX
GenF4.menu.pnum.GENERIC_F479IITX.build.product_line=STM32F479xx
GenF4.menu.pnum.GENERIC_F479IITX.build.variant=STM32F4xx/F469I(E-G-I)(H-T)_F479I(G-I)(H-T)
GenF4.menu.pnum.GENERIC_F479IITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F479.svd

