# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic H523RCTx
GenH5.menu.pnum.GENERIC_H523RCTX=Generic H523RCTx
GenH5.menu.pnum.GENERIC_H523RCTX.upload.maximum_size=262144
GenH5.menu.pnum.GENERIC_H523RCTX.upload.maximum_data_size=278528
GenH5.menu.pnum.GENERIC_H523RCTX.build.board=GENERIC_H523RCTX
GenH5.menu.pnum.GENERIC_H523RCTX.build.product_line=STM32H523xx
GenH5.menu.pnum.GENERIC_H523RCTX.build.variant=STM32H5xx/H523R(C-E)T_H533RET
GenH5.menu.pnum.GENERIC_H523RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H523.svd

# Generic H523RETx
GenH5.menu.pnum.GENERIC_H523RETX=Generic H523RETx
GenH5.menu.pnum.GENERIC_H523RETX.upload.maximum_size=524288
GenH5.menu.pnum.GENERIC_H523RETX.upload.maximum_data_size=278528
GenH5.menu.pnum.GENERIC_H523RETX.build.board=GENERIC_H523RETX
GenH5.menu.pnum.GENERIC_H523RETX.build.product_line=STM32H523xx
GenH5.menu.pnum.GENERIC_H523RETX.build.variant=STM32H5xx/H523R(C-E)T_H533RET
GenH5.menu.pnum.GENERIC_H523RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H523.svd

# Generic H533RETx
GenH5.menu.pnum.GENERIC_H533RETX=Generic H533RETx
GenH5.menu.pnum.GENERIC_H533RETX.upload.maximum_size=524288
GenH5.menu.pnum.GENERIC_H533RETX.upload.maximum_data_size=278528
GenH5.menu.pnum.GENERIC_H533RETX.build.board=GENERIC_H533RETX
GenH5.menu.pnum.GENERIC_H533RETX.build.product_line=STM32H533xx
GenH5.menu.pnum.GENERIC_H533RETX.build.variant=STM32H5xx/H523R(C-E)T_H533RET
GenH5.menu.pnum.GENERIC_H533RETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32H5xx/STM32H533.svd

