# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L151R6Hx
GenL1.menu.pnum.GENERIC_L151R6HX=Generic L151R6Hx
GenL1.menu.pnum.GENERIC_L151R6HX.upload.maximum_size=32768
GenL1.menu.pnum.GENERIC_L151R6HX.upload.maximum_data_size=10240
GenL1.menu.pnum.GENERIC_L151R6HX.build.board=GENERIC_L151R6HX
GenL1.menu.pnum.GENERIC_L151R6HX.build.product_line=STM32L151xB
GenL1.menu.pnum.GENERIC_L151R6HX.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L151R6HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151R8Hx
GenL1.menu.pnum.GENERIC_L151R8HX=Generic L151R8Hx
GenL1.menu.pnum.GENERIC_L151R8HX.upload.maximum_size=65536
GenL1.menu.pnum.GENERIC_L151R8HX.upload.maximum_data_size=10240
GenL1.menu.pnum.GENERIC_L151R8HX.build.board=GENERIC_L151R8HX
GenL1.menu.pnum.GENERIC_L151R8HX.build.product_line=STM32L151xB
GenL1.menu.pnum.GENERIC_L151R8HX.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L151R8HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151RBHx
GenL1.menu.pnum.GENERIC_L151RBHX=Generic L151RBHx
GenL1.menu.pnum.GENERIC_L151RBHX.upload.maximum_size=131072
GenL1.menu.pnum.GENERIC_L151RBHX.upload.maximum_data_size=16384
GenL1.menu.pnum.GENERIC_L151RBHX.build.board=GENERIC_L151RBHX
GenL1.menu.pnum.GENERIC_L151RBHX.build.product_line=STM32L151xB
GenL1.menu.pnum.GENERIC_L151RBHX.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L151RBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151R6HxA
GenL1.menu.pnum.GENERIC_L151R6HXA=Generic L151R6HxA
GenL1.menu.pnum.GENERIC_L151R6HXA.upload.maximum_size=32768
GenL1.menu.pnum.GENERIC_L151R6HXA.upload.maximum_data_size=16384
GenL1.menu.pnum.GENERIC_L151R6HXA.build.board=GENERIC_L151R6HXA
GenL1.menu.pnum.GENERIC_L151R6HXA.build.product_line=STM32L151xBA
GenL1.menu.pnum.GENERIC_L151R6HXA.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L151R6HXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151R8HxA
GenL1.menu.pnum.GENERIC_L151R8HXA=Generic L151R8HxA
GenL1.menu.pnum.GENERIC_L151R8HXA.upload.maximum_size=65536
GenL1.menu.pnum.GENERIC_L151R8HXA.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L151R8HXA.build.board=GENERIC_L151R8HXA
GenL1.menu.pnum.GENERIC_L151R8HXA.build.product_line=STM32L151xBA
GenL1.menu.pnum.GENERIC_L151R8HXA.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L151R8HXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L151RBHxA
GenL1.menu.pnum.GENERIC_L151RBHXA=Generic L151RBHxA
GenL1.menu.pnum.GENERIC_L151RBHXA.upload.maximum_size=131072
GenL1.menu.pnum.GENERIC_L151RBHXA.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L151RBHXA.build.board=GENERIC_L151RBHXA
GenL1.menu.pnum.GENERIC_L151RBHXA.build.product_line=STM32L151xBA
GenL1.menu.pnum.GENERIC_L151RBHXA.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L151RBHXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L151.svd

# Generic L152R6Hx
GenL1.menu.pnum.GENERIC_L152R6HX=Generic L152R6Hx
GenL1.menu.pnum.GENERIC_L152R6HX.upload.maximum_size=32768
GenL1.menu.pnum.GENERIC_L152R6HX.upload.maximum_data_size=10240
GenL1.menu.pnum.GENERIC_L152R6HX.build.board=GENERIC_L152R6HX
GenL1.menu.pnum.GENERIC_L152R6HX.build.product_line=STM32L152xB
GenL1.menu.pnum.GENERIC_L152R6HX.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L152R6HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L152R8Hx
GenL1.menu.pnum.GENERIC_L152R8HX=Generic L152R8Hx
GenL1.menu.pnum.GENERIC_L152R8HX.upload.maximum_size=65536
GenL1.menu.pnum.GENERIC_L152R8HX.upload.maximum_data_size=10240
GenL1.menu.pnum.GENERIC_L152R8HX.build.board=GENERIC_L152R8HX
GenL1.menu.pnum.GENERIC_L152R8HX.build.product_line=STM32L152xB
GenL1.menu.pnum.GENERIC_L152R8HX.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L152R8HX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L152RBHx
GenL1.menu.pnum.GENERIC_L152RBHX=Generic L152RBHx
GenL1.menu.pnum.GENERIC_L152RBHX.upload.maximum_size=131072
GenL1.menu.pnum.GENERIC_L152RBHX.upload.maximum_data_size=16384
GenL1.menu.pnum.GENERIC_L152RBHX.build.board=GENERIC_L152RBHX
GenL1.menu.pnum.GENERIC_L152RBHX.build.product_line=STM32L152xB
GenL1.menu.pnum.GENERIC_L152RBHX.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L152RBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L152R6HxA
GenL1.menu.pnum.GENERIC_L152R6HXA=Generic L152R6HxA
GenL1.menu.pnum.GENERIC_L152R6HXA.upload.maximum_size=32768
GenL1.menu.pnum.GENERIC_L152R6HXA.upload.maximum_data_size=16384
GenL1.menu.pnum.GENERIC_L152R6HXA.build.board=GENERIC_L152R6HXA
GenL1.menu.pnum.GENERIC_L152R6HXA.build.product_line=STM32L152xBA
GenL1.menu.pnum.GENERIC_L152R6HXA.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L152R6HXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L152R8HxA
GenL1.menu.pnum.GENERIC_L152R8HXA=Generic L152R8HxA
GenL1.menu.pnum.GENERIC_L152R8HXA.upload.maximum_size=65536
GenL1.menu.pnum.GENERIC_L152R8HXA.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L152R8HXA.build.board=GENERIC_L152R8HXA
GenL1.menu.pnum.GENERIC_L152R8HXA.build.product_line=STM32L152xBA
GenL1.menu.pnum.GENERIC_L152R8HXA.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L152R8HXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

# Generic L152RBHxA
GenL1.menu.pnum.GENERIC_L152RBHXA=Generic L152RBHxA
GenL1.menu.pnum.GENERIC_L152RBHXA.upload.maximum_size=131072
GenL1.menu.pnum.GENERIC_L152RBHXA.upload.maximum_data_size=32768
GenL1.menu.pnum.GENERIC_L152RBHXA.build.board=GENERIC_L152RBHXA
GenL1.menu.pnum.GENERIC_L152RBHXA.build.product_line=STM32L152xBA
GenL1.menu.pnum.GENERIC_L152RBHXA.build.variant=STM32L1xx/L151R(6-8-B)Hx(A)_L152R(6-8-B)Hx(A)
GenL1.menu.pnum.GENERIC_L152RBHXA.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L1xx/STM32L152.svd

