# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U575ZGTx
GenU5.menu.pnum.GENERIC_U575ZGTX=Generic U575ZGTx
GenU5.menu.pnum.GENERIC_U575ZGTX.upload.maximum_size=1048576
GenU5.menu.pnum.GENERIC_U575ZGTX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575ZGTX.build.board=GENERIC_U575ZGTX
GenU5.menu.pnum.GENERIC_U575ZGTX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575ZGTX.build.variant=STM32U5xx/U575Z(G-I)T_U585ZIT
GenU5.menu.pnum.GENERIC_U575ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U575ZITx
GenU5.menu.pnum.GENERIC_U575ZITX=Generic U575ZITx
GenU5.menu.pnum.GENERIC_U575ZITX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U575ZITX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U575ZITX.build.board=GENERIC_U575ZITX
GenU5.menu.pnum.GENERIC_U575ZITX.build.product_line=STM32U575xx
GenU5.menu.pnum.GENERIC_U575ZITX.build.variant=STM32U5xx/U575Z(G-I)T_U585ZIT
GenU5.menu.pnum.GENERIC_U575ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U575.svd

# Generic U585ZITx
GenU5.menu.pnum.GENERIC_U585ZITX=Generic U585ZITx
GenU5.menu.pnum.GENERIC_U585ZITX.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U585ZITX.upload.maximum_data_size=804864
GenU5.menu.pnum.GENERIC_U585ZITX.build.board=GENERIC_U585ZITX
GenU5.menu.pnum.GENERIC_U585ZITX.build.product_line=STM32U585xx
GenU5.menu.pnum.GENERIC_U585ZITX.build.variant=STM32U5xx/U575Z(G-I)T_U585ZIT
GenU5.menu.pnum.GENERIC_U585ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U585.svd

