# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L433VCIx
GenL4.menu.pnum.GENERIC_L433VCIX=Generic L433VCIx
GenL4.menu.pnum.GENERIC_L433VCIX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L433VCIX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433VCIX.build.board=GENERIC_L433VCIX
GenL4.menu.pnum.GENERIC_L433VCIX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433VCIX.build.variant=STM32L4xx/L433VC(I-T)_L443VC(I-T)
GenL4.menu.pnum.GENERIC_L433VCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L433VCTx
GenL4.menu.pnum.GENERIC_L433VCTX=Generic L433VCTx
GenL4.menu.pnum.GENERIC_L433VCTX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L433VCTX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L433VCTX.build.board=GENERIC_L433VCTX
GenL4.menu.pnum.GENERIC_L433VCTX.build.product_line=STM32L433xx
GenL4.menu.pnum.GENERIC_L433VCTX.build.variant=STM32L4xx/L433VC(I-T)_L443VC(I-T)
GenL4.menu.pnum.GENERIC_L433VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L433.svd

# Generic L443VCIx
GenL4.menu.pnum.GENERIC_L443VCIX=Generic L443VCIx
GenL4.menu.pnum.GENERIC_L443VCIX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L443VCIX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L443VCIX.build.board=GENERIC_L443VCIX
GenL4.menu.pnum.GENERIC_L443VCIX.build.product_line=STM32L443xx
GenL4.menu.pnum.GENERIC_L443VCIX.build.variant=STM32L4xx/L433VC(I-T)_L443VC(I-T)
GenL4.menu.pnum.GENERIC_L443VCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L443.svd

# Generic L443VCTx
GenL4.menu.pnum.GENERIC_L443VCTX=Generic L443VCTx
GenL4.menu.pnum.GENERIC_L443VCTX.upload.maximum_size=262144
GenL4.menu.pnum.GENERIC_L443VCTX.upload.maximum_data_size=65536
GenL4.menu.pnum.GENERIC_L443VCTX.build.board=GENERIC_L443VCTX
GenL4.menu.pnum.GENERIC_L443VCTX.build.product_line=STM32L443xx
GenL4.menu.pnum.GENERIC_L443VCTX.build.variant=STM32L4xx/L433VC(I-T)_L443VC(I-T)
GenL4.menu.pnum.GENERIC_L443VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L443.svd

