# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U599ZIYxQ
GenU5.menu.pnum.GENERIC_U599ZIYXQ=Generic U599ZIYxQ
GenU5.menu.pnum.GENERIC_U599ZIYXQ.upload.maximum_size=2097152
GenU5.menu.pnum.GENERIC_U599ZIYXQ.upload.maximum_data_size=2574336
GenU5.menu.pnum.GENERIC_U599ZIYXQ.build.board=GENERIC_U599ZIYXQ
GenU5.menu.pnum.GENERIC_U599ZIYXQ.build.product_line=STM32U599xx
GenU5.menu.pnum.GENERIC_U599ZIYXQ.build.variant=STM32U5xx/U599Z(I-J)YxQ_U5A9ZJYxQ
GenU5.menu.pnum.GENERIC_U599ZIYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U599.svd

# Generic U599ZJYxQ
GenU5.menu.pnum.GENERIC_U599ZJYXQ=Generic U599ZJYxQ
GenU5.menu.pnum.GENERIC_U599ZJYXQ.upload.maximum_size=4194304
GenU5.menu.pnum.GENERIC_U599ZJYXQ.upload.maximum_data_size=2574336
GenU5.menu.pnum.GENERIC_U599ZJYXQ.build.board=GENERIC_U599ZJYXQ
GenU5.menu.pnum.GENERIC_U599ZJYXQ.build.product_line=STM32U599xx
GenU5.menu.pnum.GENERIC_U599ZJYXQ.build.variant=STM32U5xx/U599Z(I-J)YxQ_U5A9ZJYxQ
GenU5.menu.pnum.GENERIC_U599ZJYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U599.svd

# Generic U5A9ZJYxQ
GenU5.menu.pnum.GENERIC_U5A9ZJYXQ=Generic U5A9ZJYxQ
GenU5.menu.pnum.GENERIC_U5A9ZJYXQ.upload.maximum_size=4194304
GenU5.menu.pnum.GENERIC_U5A9ZJYXQ.upload.maximum_data_size=2574336
GenU5.menu.pnum.GENERIC_U5A9ZJYXQ.build.board=GENERIC_U5A9ZJYXQ
GenU5.menu.pnum.GENERIC_U5A9ZJYXQ.build.product_line=STM32U5A9xx
GenU5.menu.pnum.GENERIC_U5A9ZJYXQ.build.variant=STM32U5xx/U599Z(I-J)YxQ_U5A9ZJYxQ
GenU5.menu.pnum.GENERIC_U5A9ZJYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U5A9.svd

