# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic U535NCYxQ
GenU5.menu.pnum.GENERIC_U535NCYXQ=Generic U535NCYxQ
GenU5.menu.pnum.GENERIC_U535NCYXQ.upload.maximum_size=262144
GenU5.menu.pnum.GENERIC_U535NCYXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535NCYXQ.build.board=GENERIC_U535NCYXQ
GenU5.menu.pnum.GENERIC_U535NCYXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535NCYXQ.build.variant=STM32U5xx/U535N(C-E)YxQ_U545NEYxQ
GenU5.menu.pnum.GENERIC_U535NCYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U535NEYxQ
GenU5.menu.pnum.GENERIC_U535NEYXQ=Generic U535NEYxQ
GenU5.menu.pnum.GENERIC_U535NEYXQ.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U535NEYXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U535NEYXQ.build.board=GENERIC_U535NEYXQ
GenU5.menu.pnum.GENERIC_U535NEYXQ.build.product_line=STM32U535xx
GenU5.menu.pnum.GENERIC_U535NEYXQ.build.variant=STM32U5xx/U535N(C-E)YxQ_U545NEYxQ
GenU5.menu.pnum.GENERIC_U535NEYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U535.svd

# Generic U545NEYxQ
GenU5.menu.pnum.GENERIC_U545NEYXQ=Generic U545NEYxQ
GenU5.menu.pnum.GENERIC_U545NEYXQ.upload.maximum_size=524288
GenU5.menu.pnum.GENERIC_U545NEYXQ.upload.maximum_data_size=280576
GenU5.menu.pnum.GENERIC_U545NEYXQ.build.board=GENERIC_U545NEYXQ
GenU5.menu.pnum.GENERIC_U545NEYXQ.build.product_line=STM32U545xx
GenU5.menu.pnum.GENERIC_U545NEYXQ.build.variant=STM32U5xx/U535N(C-E)YxQ_U545NEYxQ
GenU5.menu.pnum.GENERIC_U545NEYXQ.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32U5xx/STM32U545.svd

