# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F427VGTx
GenF4.menu.pnum.GENERIC_F427VGTX=Generic F427VGTx
GenF4.menu.pnum.GENERIC_F427VGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F427VGTX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F427VGTX.build.board=GENERIC_F427VGTX
GenF4.menu.pnum.GENERIC_F427VGTX.build.product_line=STM32F427xx
GenF4.menu.pnum.GENERIC_F427VGTX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F427VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F427.svd

# Generic F427VITx
GenF4.menu.pnum.GENERIC_F427VITX=Generic F427VITx
GenF4.menu.pnum.GENERIC_F427VITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F427VITX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F427VITX.build.board=GENERIC_F427VITX
GenF4.menu.pnum.GENERIC_F427VITX.build.product_line=STM32F427xx
GenF4.menu.pnum.GENERIC_F427VITX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F427VITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F427.svd

# Generic F429VETx
GenF4.menu.pnum.GENERIC_F429VETX=Generic F429VETx
GenF4.menu.pnum.GENERIC_F429VETX.upload.maximum_size=524288
GenF4.menu.pnum.GENERIC_F429VETX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429VETX.build.board=GENERIC_F429VETX
GenF4.menu.pnum.GENERIC_F429VETX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429VETX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F429VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F429VGTx
GenF4.menu.pnum.GENERIC_F429VGTX=Generic F429VGTx
GenF4.menu.pnum.GENERIC_F429VGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F429VGTX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429VGTX.build.board=GENERIC_F429VGTX
GenF4.menu.pnum.GENERIC_F429VGTX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429VGTX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F429VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F429VITx
GenF4.menu.pnum.GENERIC_F429VITX=Generic F429VITx
GenF4.menu.pnum.GENERIC_F429VITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F429VITX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F429VITX.build.board=GENERIC_F429VITX
GenF4.menu.pnum.GENERIC_F429VITX.build.product_line=STM32F429xx
GenF4.menu.pnum.GENERIC_F429VITX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F429VITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F429.svd

# Generic F437VGTx
GenF4.menu.pnum.GENERIC_F437VGTX=Generic F437VGTx
GenF4.menu.pnum.GENERIC_F437VGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F437VGTX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F437VGTX.build.board=GENERIC_F437VGTX
GenF4.menu.pnum.GENERIC_F437VGTX.build.product_line=STM32F437xx
GenF4.menu.pnum.GENERIC_F437VGTX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F437VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F437.svd

# Generic F437VITx
GenF4.menu.pnum.GENERIC_F437VITX=Generic F437VITx
GenF4.menu.pnum.GENERIC_F437VITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F437VITX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F437VITX.build.board=GENERIC_F437VITX
GenF4.menu.pnum.GENERIC_F437VITX.build.product_line=STM32F437xx
GenF4.menu.pnum.GENERIC_F437VITX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F437VITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F437.svd

# Generic F439VGTx
GenF4.menu.pnum.GENERIC_F439VGTX=Generic F439VGTx
GenF4.menu.pnum.GENERIC_F439VGTX.upload.maximum_size=1048576
GenF4.menu.pnum.GENERIC_F439VGTX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F439VGTX.build.board=GENERIC_F439VGTX
GenF4.menu.pnum.GENERIC_F439VGTX.build.product_line=STM32F439xx
GenF4.menu.pnum.GENERIC_F439VGTX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F439VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F439.svd

# Generic F439VITx
GenF4.menu.pnum.GENERIC_F439VITX=Generic F439VITx
GenF4.menu.pnum.GENERIC_F439VITX.upload.maximum_size=2097152
GenF4.menu.pnum.GENERIC_F439VITX.upload.maximum_data_size=196608
GenF4.menu.pnum.GENERIC_F439VITX.build.board=GENERIC_F439VITX
GenF4.menu.pnum.GENERIC_F439VITX.build.product_line=STM32F439xx
GenF4.menu.pnum.GENERIC_F439VITX.build.variant=STM32F4xx/F427V(G-I)T_F429V(E-G-I)T_F437V(G-I)T_F439V(G-I)T
GenF4.menu.pnum.GENERIC_F439VITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F4xx/STM32F439.svd

