# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F723ICKx
GenF7.menu.pnum.GENERIC_F723ICKX=Generic F723ICKx
GenF7.menu.pnum.GENERIC_F723ICKX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F723ICKX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723ICKX.build.board=GENERIC_F723ICKX
GenF7.menu.pnum.GENERIC_F723ICKX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723ICKX.build.variant=STM32F7xx/F723I(C-E)(K-T)_F730I8K_F733IE(K-T)
GenF7.menu.pnum.GENERIC_F723ICKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723IEKx
GenF7.menu.pnum.GENERIC_F723IEKX=Generic F723IEKx
GenF7.menu.pnum.GENERIC_F723IEKX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F723IEKX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723IEKX.build.board=GENERIC_F723IEKX
GenF7.menu.pnum.GENERIC_F723IEKX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723IEKX.build.variant=STM32F7xx/F723I(C-E)(K-T)_F730I8K_F733IE(K-T)
GenF7.menu.pnum.GENERIC_F723IEKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723ICTx
GenF7.menu.pnum.GENERIC_F723ICTX=Generic F723ICTx
GenF7.menu.pnum.GENERIC_F723ICTX.upload.maximum_size=262144
GenF7.menu.pnum.GENERIC_F723ICTX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723ICTX.build.board=GENERIC_F723ICTX
GenF7.menu.pnum.GENERIC_F723ICTX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723ICTX.build.variant=STM32F7xx/F723I(C-E)(K-T)_F730I8K_F733IE(K-T)
GenF7.menu.pnum.GENERIC_F723ICTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F723IETx
GenF7.menu.pnum.GENERIC_F723IETX=Generic F723IETx
GenF7.menu.pnum.GENERIC_F723IETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F723IETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F723IETX.build.board=GENERIC_F723IETX
GenF7.menu.pnum.GENERIC_F723IETX.build.product_line=STM32F723xx
GenF7.menu.pnum.GENERIC_F723IETX.build.variant=STM32F7xx/F723I(C-E)(K-T)_F730I8K_F733IE(K-T)
GenF7.menu.pnum.GENERIC_F723IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F723.svd

# Generic F730I8Kx
GenF7.menu.pnum.GENERIC_F730I8KX=Generic F730I8Kx
GenF7.menu.pnum.GENERIC_F730I8KX.upload.maximum_size=65536
GenF7.menu.pnum.GENERIC_F730I8KX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F730I8KX.build.board=GENERIC_F730I8KX
GenF7.menu.pnum.GENERIC_F730I8KX.build.product_line=STM32F730xx
GenF7.menu.pnum.GENERIC_F730I8KX.build.variant=STM32F7xx/F723I(C-E)(K-T)_F730I8K_F733IE(K-T)
GenF7.menu.pnum.GENERIC_F730I8KX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F730.svd

# Generic F733IEKx
GenF7.menu.pnum.GENERIC_F733IEKX=Generic F733IEKx
GenF7.menu.pnum.GENERIC_F733IEKX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F733IEKX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F733IEKX.build.board=GENERIC_F733IEKX
GenF7.menu.pnum.GENERIC_F733IEKX.build.product_line=STM32F733xx
GenF7.menu.pnum.GENERIC_F733IEKX.build.variant=STM32F7xx/F723I(C-E)(K-T)_F730I8K_F733IE(K-T)
GenF7.menu.pnum.GENERIC_F733IEKX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F733.svd

# Generic F733IETx
GenF7.menu.pnum.GENERIC_F733IETX=Generic F733IETx
GenF7.menu.pnum.GENERIC_F733IETX.upload.maximum_size=524288
GenF7.menu.pnum.GENERIC_F733IETX.upload.maximum_data_size=196608
GenF7.menu.pnum.GENERIC_F733IETX.build.board=GENERIC_F733IETX
GenF7.menu.pnum.GENERIC_F733IETX.build.product_line=STM32F733xx
GenF7.menu.pnum.GENERIC_F733IETX.build.variant=STM32F7xx/F723I(C-E)(K-T)_F730I8K_F733IE(K-T)
GenF7.menu.pnum.GENERIC_F733IETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F7xx/STM32F733.svd

