# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F302VDHx
GenF3.menu.pnum.GENERIC_F302VDHX=Generic F302VDHx
GenF3.menu.pnum.GENERIC_F302VDHX.upload.maximum_size=393216
GenF3.menu.pnum.GENERIC_F302VDHX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F302VDHX.build.board=GENERIC_F302VDHX
GenF3.menu.pnum.GENERIC_F302VDHX.build.product_line=STM32F302xE
GenF3.menu.pnum.GENERIC_F302VDHX.build.variant=STM32F3xx/F302V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F302VDHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F302.svd

# Generic F302VEHx
GenF3.menu.pnum.GENERIC_F302VEHX=Generic F302VEHx
GenF3.menu.pnum.GENERIC_F302VEHX.upload.maximum_size=524288
GenF3.menu.pnum.GENERIC_F302VEHX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F302VEHX.build.board=GENERIC_F302VEHX
GenF3.menu.pnum.GENERIC_F302VEHX.build.product_line=STM32F302xE
GenF3.menu.pnum.GENERIC_F302VEHX.build.variant=STM32F3xx/F302V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F302VEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F302.svd

# Generic F302VDTx
GenF3.menu.pnum.GENERIC_F302VDTX=Generic F302VDTx
GenF3.menu.pnum.GENERIC_F302VDTX.upload.maximum_size=393216
GenF3.menu.pnum.GENERIC_F302VDTX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F302VDTX.build.board=GENERIC_F302VDTX
GenF3.menu.pnum.GENERIC_F302VDTX.build.product_line=STM32F302xE
GenF3.menu.pnum.GENERIC_F302VDTX.build.variant=STM32F3xx/F302V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F302VDTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F302.svd

# Generic F302VETx
GenF3.menu.pnum.GENERIC_F302VETX=Generic F302VETx
GenF3.menu.pnum.GENERIC_F302VETX.upload.maximum_size=524288
GenF3.menu.pnum.GENERIC_F302VETX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F302VETX.build.board=GENERIC_F302VETX
GenF3.menu.pnum.GENERIC_F302VETX.build.product_line=STM32F302xE
GenF3.menu.pnum.GENERIC_F302VETX.build.variant=STM32F3xx/F302V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F302VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F302.svd

