# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F303VDHx
GenF3.menu.pnum.GENERIC_F303VDHX=Generic F303VDHx
GenF3.menu.pnum.GENERIC_F303VDHX.upload.maximum_size=393216
GenF3.menu.pnum.GENERIC_F303VDHX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F303VDHX.build.board=GENERIC_F303VDHX
GenF3.menu.pnum.GENERIC_F303VDHX.build.product_line=STM32F303xE
GenF3.menu.pnum.GENERIC_F303VDHX.build.variant=STM32F3xx/F303V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F303VDHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F303VEHx
GenF3.menu.pnum.GENERIC_F303VEHX=Generic F303VEHx
GenF3.menu.pnum.GENERIC_F303VEHX.upload.maximum_size=524288
GenF3.menu.pnum.GENERIC_F303VEHX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F303VEHX.build.board=GENERIC_F303VEHX
GenF3.menu.pnum.GENERIC_F303VEHX.build.product_line=STM32F303xE
GenF3.menu.pnum.GENERIC_F303VEHX.build.variant=STM32F3xx/F303V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F303VEHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F303VDTx
GenF3.menu.pnum.GENERIC_F303VDTX=Generic F303VDTx
GenF3.menu.pnum.GENERIC_F303VDTX.upload.maximum_size=393216
GenF3.menu.pnum.GENERIC_F303VDTX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F303VDTX.build.board=GENERIC_F303VDTX
GenF3.menu.pnum.GENERIC_F303VDTX.build.product_line=STM32F303xE
GenF3.menu.pnum.GENERIC_F303VDTX.build.variant=STM32F3xx/F303V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F303VDTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F303VETx
GenF3.menu.pnum.GENERIC_F303VETX=Generic F303VETx
GenF3.menu.pnum.GENERIC_F303VETX.upload.maximum_size=524288
GenF3.menu.pnum.GENERIC_F303VETX.upload.maximum_data_size=65536
GenF3.menu.pnum.GENERIC_F303VETX.build.board=GENERIC_F303VETX
GenF3.menu.pnum.GENERIC_F303VETX.build.product_line=STM32F303xE
GenF3.menu.pnum.GENERIC_F303VETX.build.variant=STM32F3xx/F303V(D-E)(H-T)
GenF3.menu.pnum.GENERIC_F303VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

