# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L072CBYx
GenL0.menu.pnum.GENERIC_L072CBYX=Generic L072CBYx
GenL0.menu.pnum.GENERIC_L072CBYX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L072CBYX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072CBYX.build.board=GENERIC_L072CBYX
GenL0.menu.pnum.GENERIC_L072CBYX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072CBYX.build.variant=STM32L0xx/L072CBY_L072CZ(E-Y)_L073CZY_L082CZY
GenL0.menu.pnum.GENERIC_L072CBYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072CZYx
GenL0.menu.pnum.GENERIC_L072CZYX=Generic L072CZYx
GenL0.menu.pnum.GENERIC_L072CZYX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072CZYX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072CZYX.build.board=GENERIC_L072CZYX
GenL0.menu.pnum.GENERIC_L072CZYX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072CZYX.build.variant=STM32L0xx/L072CBY_L072CZ(E-Y)_L073CZY_L082CZY
GenL0.menu.pnum.GENERIC_L072CZYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072CZEx
GenL0.menu.pnum.GENERIC_L072CZEX=Generic L072CZEx
GenL0.menu.pnum.GENERIC_L072CZEX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072CZEX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072CZEX.build.board=GENERIC_L072CZEX
GenL0.menu.pnum.GENERIC_L072CZEX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072CZEX.build.variant=STM32L0xx/L072CBY_L072CZ(E-Y)_L073CZY_L082CZY
GenL0.menu.pnum.GENERIC_L072CZEX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L073CZYx
GenL0.menu.pnum.GENERIC_L073CZYX=Generic L073CZYx
GenL0.menu.pnum.GENERIC_L073CZYX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L073CZYX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073CZYX.build.board=GENERIC_L073CZYX
GenL0.menu.pnum.GENERIC_L073CZYX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073CZYX.build.variant=STM32L0xx/L072CBY_L072CZ(E-Y)_L073CZY_L082CZY
GenL0.menu.pnum.GENERIC_L073CZYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L082CZYx
GenL0.menu.pnum.GENERIC_L082CZYX=Generic L082CZYx
GenL0.menu.pnum.GENERIC_L082CZYX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L082CZYX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L082CZYX.build.board=GENERIC_L082CZYX
GenL0.menu.pnum.GENERIC_L082CZYX.build.product_line=STM32L082xx
GenL0.menu.pnum.GENERIC_L082CZYX.build.variant=STM32L0xx/L072CBY_L072CZ(E-Y)_L073CZY_L082CZY
GenL0.menu.pnum.GENERIC_L082CZYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

