# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic G473CBTx
GenG4.menu.pnum.GENERIC_G473CBTX=Generic G473CBTx
GenG4.menu.pnum.GENERIC_G473CBTX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G473CBTX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G473CBTX.build.board=GENERIC_G473CBTX
GenG4.menu.pnum.GENERIC_G473CBTX.build.product_line=STM32G473xx
GenG4.menu.pnum.GENERIC_G473CBTX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G473CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G473.svd

# Generic G473CCTx
GenG4.menu.pnum.GENERIC_G473CCTX=Generic G473CCTx
GenG4.menu.pnum.GENERIC_G473CCTX.upload.maximum_size=262144
GenG4.menu.pnum.GENERIC_G473CCTX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G473CCTX.build.board=GENERIC_G473CCTX
GenG4.menu.pnum.GENERIC_G473CCTX.build.product_line=STM32G473xx
GenG4.menu.pnum.GENERIC_G473CCTX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G473CCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G473.svd

# Generic G473CETx
GenG4.menu.pnum.GENERIC_G473CETX=Generic G473CETx
GenG4.menu.pnum.GENERIC_G473CETX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G473CETX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G473CETX.build.board=GENERIC_G473CETX
GenG4.menu.pnum.GENERIC_G473CETX.build.product_line=STM32G473xx
GenG4.menu.pnum.GENERIC_G473CETX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G473CETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G473.svd

# Generic G474CBTx
GenG4.menu.pnum.GENERIC_G474CBTX=Generic G474CBTx
GenG4.menu.pnum.GENERIC_G474CBTX.upload.maximum_size=131072
GenG4.menu.pnum.GENERIC_G474CBTX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G474CBTX.build.board=GENERIC_G474CBTX
GenG4.menu.pnum.GENERIC_G474CBTX.build.product_line=STM32G474xx
GenG4.menu.pnum.GENERIC_G474CBTX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G474CBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G474.svd

# Generic G474CCTx
GenG4.menu.pnum.GENERIC_G474CCTX=Generic G474CCTx
GenG4.menu.pnum.GENERIC_G474CCTX.upload.maximum_size=262144
GenG4.menu.pnum.GENERIC_G474CCTX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G474CCTX.build.board=GENERIC_G474CCTX
GenG4.menu.pnum.GENERIC_G474CCTX.build.product_line=STM32G474xx
GenG4.menu.pnum.GENERIC_G474CCTX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G474CCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G474.svd

# Generic G474CETx
GenG4.menu.pnum.GENERIC_G474CETX=Generic G474CETx
GenG4.menu.pnum.GENERIC_G474CETX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G474CETX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G474CETX.build.board=GENERIC_G474CETX
GenG4.menu.pnum.GENERIC_G474CETX.build.product_line=STM32G474xx
GenG4.menu.pnum.GENERIC_G474CETX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G474CETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G474.svd

# Generic G483CETx
GenG4.menu.pnum.GENERIC_G483CETX=Generic G483CETx
GenG4.menu.pnum.GENERIC_G483CETX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G483CETX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G483CETX.build.board=GENERIC_G483CETX
GenG4.menu.pnum.GENERIC_G483CETX.build.product_line=STM32G483xx
GenG4.menu.pnum.GENERIC_G483CETX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G483CETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G483.svd

# Generic G484CETx
GenG4.menu.pnum.GENERIC_G484CETX=Generic G484CETx
GenG4.menu.pnum.GENERIC_G484CETX.upload.maximum_size=524288
GenG4.menu.pnum.GENERIC_G484CETX.upload.maximum_data_size=131072
GenG4.menu.pnum.GENERIC_G484CETX.build.board=GENERIC_G484CETX
GenG4.menu.pnum.GENERIC_G484CETX.build.product_line=STM32G484xx
GenG4.menu.pnum.GENERIC_G484CETX.build.variant=STM32G4xx/G473C(B-C-E)T_G474C(B-C-E)T_G483CET_G484CET
GenG4.menu.pnum.GENERIC_G484CETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32G4xx/STM32G484.svd

