# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L071KBUx
GenL0.menu.pnum.GENERIC_L071KBUX=Generic L071KBUx
GenL0.menu.pnum.GENERIC_L071KBUX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L071KBUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071KBUX.build.board=GENERIC_L071KBUX
GenL0.menu.pnum.GENERIC_L071KBUX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071KBUX.build.variant=STM32L0xx/L071K(8-B-Z)U_L081KZU
GenL0.menu.pnum.GENERIC_L071KBUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071KZUx
GenL0.menu.pnum.GENERIC_L071KZUX=Generic L071KZUx
GenL0.menu.pnum.GENERIC_L071KZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L071KZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071KZUX.build.board=GENERIC_L071KZUX
GenL0.menu.pnum.GENERIC_L071KZUX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071KZUX.build.variant=STM32L0xx/L071K(8-B-Z)U_L081KZU
GenL0.menu.pnum.GENERIC_L071KZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L071K8Ux
GenL0.menu.pnum.GENERIC_L071K8UX=Generic L071K8Ux
GenL0.menu.pnum.GENERIC_L071K8UX.upload.maximum_size=65536
GenL0.menu.pnum.GENERIC_L071K8UX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L071K8UX.build.board=GENERIC_L071K8UX
GenL0.menu.pnum.GENERIC_L071K8UX.build.product_line=STM32L071xx
GenL0.menu.pnum.GENERIC_L071K8UX.build.variant=STM32L0xx/L071K(8-B-Z)U_L081KZU
GenL0.menu.pnum.GENERIC_L071K8UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

# Generic L081KZUx
GenL0.menu.pnum.GENERIC_L081KZUX=Generic L081KZUx
GenL0.menu.pnum.GENERIC_L081KZUX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L081KZUX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L081KZUX.build.board=GENERIC_L081KZUX
GenL0.menu.pnum.GENERIC_L081KZUX.build.product_line=STM32L081xx
GenL0.menu.pnum.GENERIC_L081KZUX.build.variant=STM32L0xx/L071K(8-B-Z)U_L081KZU
GenL0.menu.pnum.GENERIC_L081KZUX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x1.svd

