# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic C071R8TxN
GenC0.menu.pnum.GENERIC_C071R8TXN=Generic C071R8TxN
GenC0.menu.pnum.GENERIC_C071R8TXN.upload.maximum_size=65536
GenC0.menu.pnum.GENERIC_C071R8TXN.upload.maximum_data_size=24576
GenC0.menu.pnum.GENERIC_C071R8TXN.build.board=GENERIC_C071R8TXN
GenC0.menu.pnum.GENERIC_C071R8TXN.build.product_line=STM32C071xx
GenC0.menu.pnum.GENERIC_C071R8TXN.build.variant=STM32C0xx/C071R8TxN_C071RB(I-T)xN
GenC0.menu.pnum.GENERIC_C071R8TXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C071.svd

# Generic C071RBIxN
GenC0.menu.pnum.GENERIC_C071RBIXN=Generic C071RBIxN
GenC0.menu.pnum.GENERIC_C071RBIXN.upload.maximum_size=131072
GenC0.menu.pnum.GENERIC_C071RBIXN.upload.maximum_data_size=24576
GenC0.menu.pnum.GENERIC_C071RBIXN.build.board=GENERIC_C071RBIXN
GenC0.menu.pnum.GENERIC_C071RBIXN.build.product_line=STM32C071xx
GenC0.menu.pnum.GENERIC_C071RBIXN.build.variant=STM32C0xx/C071R8TxN_C071RB(I-T)xN
GenC0.menu.pnum.GENERIC_C071RBIXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C071.svd

# Generic C071RBTxN
GenC0.menu.pnum.GENERIC_C071RBTXN=Generic C071RBTxN
GenC0.menu.pnum.GENERIC_C071RBTXN.upload.maximum_size=131072
GenC0.menu.pnum.GENERIC_C071RBTXN.upload.maximum_data_size=24576
GenC0.menu.pnum.GENERIC_C071RBTXN.build.board=GENERIC_C071RBTXN
GenC0.menu.pnum.GENERIC_C071RBTXN.build.product_line=STM32C071xx
GenC0.menu.pnum.GENERIC_C071RBTXN.build.variant=STM32C0xx/C071R8TxN_C071RB(I-T)xN
GenC0.menu.pnum.GENERIC_C071RBTXN.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32C0xx/STM32C071.svd

