# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F303VBTx
GenF3.menu.pnum.GENERIC_F303VBTX=Generic F303VBTx
GenF3.menu.pnum.GENERIC_F303VBTX.upload.maximum_size=131072
GenF3.menu.pnum.GENERIC_F303VBTX.upload.maximum_data_size=32768
GenF3.menu.pnum.GENERIC_F303VBTX.build.board=GENERIC_F303VBTX
GenF3.menu.pnum.GENERIC_F303VBTX.build.product_line=STM32F303xC
GenF3.menu.pnum.GENERIC_F303VBTX.build.variant=STM32F3xx/F303V(B-C)T
GenF3.menu.pnum.GENERIC_F303VBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

# Generic F303VCTx
GenF3.menu.pnum.GENERIC_F303VCTX=Generic F303VCTx
GenF3.menu.pnum.GENERIC_F303VCTX.upload.maximum_size=262144
GenF3.menu.pnum.GENERIC_F303VCTX.upload.maximum_data_size=40960
GenF3.menu.pnum.GENERIC_F303VCTX.build.board=GENERIC_F303VCTX
GenF3.menu.pnum.GENERIC_F303VCTX.build.product_line=STM32F303xC
GenF3.menu.pnum.GENERIC_F303VCTX.build.variant=STM32F3xx/F303V(B-C)T
GenF3.menu.pnum.GENERIC_F303VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F303.svd

