# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F103RCYx
GenF1.menu.pnum.GENERIC_F103RCYX=Generic F103RCYx
GenF1.menu.pnum.GENERIC_F103RCYX.upload.maximum_size=262144
GenF1.menu.pnum.GENERIC_F103RCYX.upload.maximum_data_size=49152
GenF1.menu.pnum.GENERIC_F103RCYX.build.board=GENERIC_F103RCYX
GenF1.menu.pnum.GENERIC_F103RCYX.build.product_line=STM32F103xE
GenF1.menu.pnum.GENERIC_F103RCYX.build.variant=STM32F1xx/F103R(C-D-E)Y
GenF1.menu.pnum.GENERIC_F103RCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F103.svd

# Generic F103RDYx
GenF1.menu.pnum.GENERIC_F103RDYX=Generic F103RDYx
GenF1.menu.pnum.GENERIC_F103RDYX.upload.maximum_size=393216
GenF1.menu.pnum.GENERIC_F103RDYX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F103RDYX.build.board=GENERIC_F103RDYX
GenF1.menu.pnum.GENERIC_F103RDYX.build.product_line=STM32F103xE
GenF1.menu.pnum.GENERIC_F103RDYX.build.variant=STM32F1xx/F103R(C-D-E)Y
GenF1.menu.pnum.GENERIC_F103RDYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F103.svd

# Generic F103REYx
GenF1.menu.pnum.GENERIC_F103REYX=Generic F103REYx
GenF1.menu.pnum.GENERIC_F103REYX.upload.maximum_size=524288
GenF1.menu.pnum.GENERIC_F103REYX.upload.maximum_data_size=65536
GenF1.menu.pnum.GENERIC_F103REYX.build.board=GENERIC_F103REYX
GenF1.menu.pnum.GENERIC_F103REYX.build.product_line=STM32F103xE
GenF1.menu.pnum.GENERIC_F103REYX.build.variant=STM32F1xx/F103R(C-D-E)Y
GenF1.menu.pnum.GENERIC_F103REYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F103.svd

