# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F373R8Tx
GenF3.menu.pnum.GENERIC_F373R8TX=Generic F373R8Tx
GenF3.menu.pnum.GENERIC_F373R8TX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F373R8TX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F373R8TX.build.board=GENERIC_F373R8TX
GenF3.menu.pnum.GENERIC_F373R8TX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373R8TX.build.variant=STM32F3xx/F373R(8-B-C)T
GenF3.menu.pnum.GENERIC_F373R8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

# Generic F373RBTx
GenF3.menu.pnum.GENERIC_F373RBTX=Generic F373RBTx
GenF3.menu.pnum.GENERIC_F373RBTX.upload.maximum_size=131072
GenF3.menu.pnum.GENERIC_F373RBTX.upload.maximum_data_size=24576
GenF3.menu.pnum.GENERIC_F373RBTX.build.board=GENERIC_F373RBTX
GenF3.menu.pnum.GENERIC_F373RBTX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373RBTX.build.variant=STM32F3xx/F373R(8-B-C)T
GenF3.menu.pnum.GENERIC_F373RBTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

# Generic F373RCTx
GenF3.menu.pnum.GENERIC_F373RCTX=Generic F373RCTx
GenF3.menu.pnum.GENERIC_F373RCTX.upload.maximum_size=262144
GenF3.menu.pnum.GENERIC_F373RCTX.upload.maximum_data_size=32768
GenF3.menu.pnum.GENERIC_F373RCTX.build.board=GENERIC_F373RCTX
GenF3.menu.pnum.GENERIC_F373RCTX.build.product_line=STM32F373xC
GenF3.menu.pnum.GENERIC_F373RCTX.build.variant=STM32F3xx/F373R(8-B-C)T
GenF3.menu.pnum.GENERIC_F373RCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F373.svd

