# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F207VCTx
GenF2.menu.pnum.GENERIC_F207VCTX=Generic F207VCTx
GenF2.menu.pnum.GENERIC_F207VCTX.upload.maximum_size=262144
GenF2.menu.pnum.GENERIC_F207VCTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F207VCTX.build.board=GENERIC_F207VCTX
GenF2.menu.pnum.GENERIC_F207VCTX.build.product_line=STM32F207xx
GenF2.menu.pnum.GENERIC_F207VCTX.build.variant=STM32F2xx/F207V(C-E-F-G)T_F217V(E-G)T
GenF2.menu.pnum.GENERIC_F207VCTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F207.svd

# Generic F207VETx
GenF2.menu.pnum.GENERIC_F207VETX=Generic F207VETx
GenF2.menu.pnum.GENERIC_F207VETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F207VETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F207VETX.build.board=GENERIC_F207VETX
GenF2.menu.pnum.GENERIC_F207VETX.build.product_line=STM32F207xx
GenF2.menu.pnum.GENERIC_F207VETX.build.variant=STM32F2xx/F207V(C-E-F-G)T_F217V(E-G)T
GenF2.menu.pnum.GENERIC_F207VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F207.svd

# Generic F207VFTx
GenF2.menu.pnum.GENERIC_F207VFTX=Generic F207VFTx
GenF2.menu.pnum.GENERIC_F207VFTX.upload.maximum_size=786432
GenF2.menu.pnum.GENERIC_F207VFTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F207VFTX.build.board=GENERIC_F207VFTX
GenF2.menu.pnum.GENERIC_F207VFTX.build.product_line=STM32F207xx
GenF2.menu.pnum.GENERIC_F207VFTX.build.variant=STM32F2xx/F207V(C-E-F-G)T_F217V(E-G)T
GenF2.menu.pnum.GENERIC_F207VFTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F207.svd

# Generic F207VGTx
GenF2.menu.pnum.GENERIC_F207VGTX=Generic F207VGTx
GenF2.menu.pnum.GENERIC_F207VGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F207VGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F207VGTX.build.board=GENERIC_F207VGTX
GenF2.menu.pnum.GENERIC_F207VGTX.build.product_line=STM32F207xx
GenF2.menu.pnum.GENERIC_F207VGTX.build.variant=STM32F2xx/F207V(C-E-F-G)T_F217V(E-G)T
GenF2.menu.pnum.GENERIC_F207VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F207.svd

# Generic F217VETx
GenF2.menu.pnum.GENERIC_F217VETX=Generic F217VETx
GenF2.menu.pnum.GENERIC_F217VETX.upload.maximum_size=524288
GenF2.menu.pnum.GENERIC_F217VETX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F217VETX.build.board=GENERIC_F217VETX
GenF2.menu.pnum.GENERIC_F217VETX.build.product_line=STM32F217xx
GenF2.menu.pnum.GENERIC_F217VETX.build.variant=STM32F2xx/F207V(C-E-F-G)T_F217V(E-G)T
GenF2.menu.pnum.GENERIC_F217VETX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F217.svd

# Generic F217VGTx
GenF2.menu.pnum.GENERIC_F217VGTX=Generic F217VGTx
GenF2.menu.pnum.GENERIC_F217VGTX.upload.maximum_size=1048576
GenF2.menu.pnum.GENERIC_F217VGTX.upload.maximum_data_size=131072
GenF2.menu.pnum.GENERIC_F217VGTX.build.board=GENERIC_F217VGTX
GenF2.menu.pnum.GENERIC_F217VGTX.build.product_line=STM32F217xx
GenF2.menu.pnum.GENERIC_F217VGTX.build.variant=STM32F2xx/F207V(C-E-F-G)T_F217V(E-G)T
GenF2.menu.pnum.GENERIC_F217VGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F2xx/STM32F217.svd

