# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F103C4Tx
GenF1.menu.pnum.GENERIC_F103C4TX=Generic F103C4Tx
GenF1.menu.pnum.GENERIC_F103C4TX.upload.maximum_size=16384
GenF1.menu.pnum.GENERIC_F103C4TX.upload.maximum_data_size=6144
GenF1.menu.pnum.GENERIC_F103C4TX.build.board=GENERIC_F103C4TX
GenF1.menu.pnum.GENERIC_F103C4TX.build.product_line=STM32F103x6
GenF1.menu.pnum.GENERIC_F103C4TX.build.variant=STM32F1xx/F103C4T_F103C6(T-U)
GenF1.menu.pnum.GENERIC_F103C4TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F103.svd

# Generic F103C6Tx
GenF1.menu.pnum.GENERIC_F103C6TX=Generic F103C6Tx
GenF1.menu.pnum.GENERIC_F103C6TX.upload.maximum_size=32768
GenF1.menu.pnum.GENERIC_F103C6TX.upload.maximum_data_size=10240
GenF1.menu.pnum.GENERIC_F103C6TX.build.board=GENERIC_F103C6TX
GenF1.menu.pnum.GENERIC_F103C6TX.build.product_line=STM32F103x6
GenF1.menu.pnum.GENERIC_F103C6TX.build.variant=STM32F1xx/F103C4T_F103C6(T-U)
GenF1.menu.pnum.GENERIC_F103C6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F103.svd

# Generic F103C6Ux
GenF1.menu.pnum.GENERIC_F103C6UX=Generic F103C6Ux
GenF1.menu.pnum.GENERIC_F103C6UX.upload.maximum_size=32768
GenF1.menu.pnum.GENERIC_F103C6UX.upload.maximum_data_size=10240
GenF1.menu.pnum.GENERIC_F103C6UX.build.board=GENERIC_F103C6UX
GenF1.menu.pnum.GENERIC_F103C6UX.build.product_line=STM32F103x6
GenF1.menu.pnum.GENERIC_F103C6UX.build.variant=STM32F1xx/F103C4T_F103C6(T-U)
GenF1.menu.pnum.GENERIC_F103C6UX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F1xx/STM32F103.svd

