# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic F301C6Tx
GenF3.menu.pnum.GENERIC_F301C6TX=Generic F301C6Tx
GenF3.menu.pnum.GENERIC_F301C6TX.upload.maximum_size=32768
GenF3.menu.pnum.GENERIC_F301C6TX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F301C6TX.build.board=GENERIC_F301C6TX
GenF3.menu.pnum.GENERIC_F301C6TX.build.product_line=STM32F301x8
GenF3.menu.pnum.GENERIC_F301C6TX.build.variant=STM32F3xx/F301C6T_F301C8(T-Y)
GenF3.menu.pnum.GENERIC_F301C6TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F301.svd

# Generic F301C8Tx
GenF3.menu.pnum.GENERIC_F301C8TX=Generic F301C8Tx
GenF3.menu.pnum.GENERIC_F301C8TX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F301C8TX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F301C8TX.build.board=GENERIC_F301C8TX
GenF3.menu.pnum.GENERIC_F301C8TX.build.product_line=STM32F301x8
GenF3.menu.pnum.GENERIC_F301C8TX.build.variant=STM32F3xx/F301C6T_F301C8(T-Y)
GenF3.menu.pnum.GENERIC_F301C8TX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F301.svd

# Generic F301C8Yx
GenF3.menu.pnum.GENERIC_F301C8YX=Generic F301C8Yx
GenF3.menu.pnum.GENERIC_F301C8YX.upload.maximum_size=65536
GenF3.menu.pnum.GENERIC_F301C8YX.upload.maximum_data_size=16384
GenF3.menu.pnum.GENERIC_F301C8YX.build.board=GENERIC_F301C8YX
GenF3.menu.pnum.GENERIC_F301C8YX.build.product_line=STM32F301x8
GenF3.menu.pnum.GENERIC_F301C8YX.build.variant=STM32F3xx/F301C6T_F301C8(T-Y)
GenF3.menu.pnum.GENERIC_F301C8YX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32F3xx/STM32F301.svd

