# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L072RBHx
GenL0.menu.pnum.GENERIC_L072RBHX=Generic L072RBHx
GenL0.menu.pnum.GENERIC_L072RBHX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L072RBHX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072RBHX.build.board=GENERIC_L072RBHX
GenL0.menu.pnum.GENERIC_L072RBHX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072RBHX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L072RBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072RZHx
GenL0.menu.pnum.GENERIC_L072RZHX=Generic L072RZHx
GenL0.menu.pnum.GENERIC_L072RZHX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072RZHX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072RZHX.build.board=GENERIC_L072RZHX
GenL0.menu.pnum.GENERIC_L072RZHX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072RZHX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L072RZHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072RBIx
GenL0.menu.pnum.GENERIC_L072RBIX=Generic L072RBIx
GenL0.menu.pnum.GENERIC_L072RBIX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L072RBIX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072RBIX.build.board=GENERIC_L072RBIX
GenL0.menu.pnum.GENERIC_L072RBIX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072RBIX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L072RBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L072RZIx
GenL0.menu.pnum.GENERIC_L072RZIX=Generic L072RZIx
GenL0.menu.pnum.GENERIC_L072RZIX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L072RZIX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L072RZIX.build.board=GENERIC_L072RZIX
GenL0.menu.pnum.GENERIC_L072RZIX.build.product_line=STM32L072xx
GenL0.menu.pnum.GENERIC_L072RZIX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L072RZIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x2.svd

# Generic L073RBHx
GenL0.menu.pnum.GENERIC_L073RBHX=Generic L073RBHx
GenL0.menu.pnum.GENERIC_L073RBHX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L073RBHX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073RBHX.build.board=GENERIC_L073RBHX
GenL0.menu.pnum.GENERIC_L073RBHX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073RBHX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L073RBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L073RZHx
GenL0.menu.pnum.GENERIC_L073RZHX=Generic L073RZHx
GenL0.menu.pnum.GENERIC_L073RZHX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L073RZHX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073RZHX.build.board=GENERIC_L073RZHX
GenL0.menu.pnum.GENERIC_L073RZHX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073RZHX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L073RZHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L073RZIx
GenL0.menu.pnum.GENERIC_L073RZIX=Generic L073RZIx
GenL0.menu.pnum.GENERIC_L073RZIX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L073RZIX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L073RZIX.build.board=GENERIC_L073RZIX
GenL0.menu.pnum.GENERIC_L073RZIX.build.product_line=STM32L073xx
GenL0.menu.pnum.GENERIC_L073RZIX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L073RZIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L083RBHx
GenL0.menu.pnum.GENERIC_L083RBHX=Generic L083RBHx
GenL0.menu.pnum.GENERIC_L083RBHX.upload.maximum_size=131072
GenL0.menu.pnum.GENERIC_L083RBHX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L083RBHX.build.board=GENERIC_L083RBHX
GenL0.menu.pnum.GENERIC_L083RBHX.build.product_line=STM32L083xx
GenL0.menu.pnum.GENERIC_L083RBHX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L083RBHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

# Generic L083RZHx
GenL0.menu.pnum.GENERIC_L083RZHX=Generic L083RZHx
GenL0.menu.pnum.GENERIC_L083RZHX.upload.maximum_size=196608
GenL0.menu.pnum.GENERIC_L083RZHX.upload.maximum_data_size=20480
GenL0.menu.pnum.GENERIC_L083RZHX.build.board=GENERIC_L083RZHX
GenL0.menu.pnum.GENERIC_L083RZHX.build.product_line=STM32L083xx
GenL0.menu.pnum.GENERIC_L083RZHX.build.variant=STM32L0xx/L072R(B-Z)(H-I)_L073RBH_L073RZ(H-I)_L083R(B-Z)H
GenL0.menu.pnum.GENERIC_L083RZHX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L0xx/STM32L0x3.svd

