# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic L4R9ZGTx
GenL4.menu.pnum.GENERIC_L4R9ZGTX=Generic L4R9ZGTx
GenL4.menu.pnum.GENERIC_L4R9ZGTX.upload.maximum_size=1048576
GenL4.menu.pnum.GENERIC_L4R9ZGTX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R9ZGTX.build.board=GENERIC_L4R9ZGTX
GenL4.menu.pnum.GENERIC_L4R9ZGTX.build.product_line=STM32L4R9xx
GenL4.menu.pnum.GENERIC_L4R9ZGTX.build.variant=STM32L4xx/L4R9Z(G-I)T_L4S9ZIT
GenL4.menu.pnum.GENERIC_L4R9ZGTX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R9.svd

# Generic L4R9ZITx
GenL4.menu.pnum.GENERIC_L4R9ZITX=Generic L4R9ZITx
GenL4.menu.pnum.GENERIC_L4R9ZITX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4R9ZITX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4R9ZITX.build.board=GENERIC_L4R9ZITX
GenL4.menu.pnum.GENERIC_L4R9ZITX.build.product_line=STM32L4R9xx
GenL4.menu.pnum.GENERIC_L4R9ZITX.build.variant=STM32L4xx/L4R9Z(G-I)T_L4S9ZIT
GenL4.menu.pnum.GENERIC_L4R9ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4R9.svd

# Generic L4S9ZITx
GenL4.menu.pnum.GENERIC_L4S9ZITX=Generic L4S9ZITx
GenL4.menu.pnum.GENERIC_L4S9ZITX.upload.maximum_size=2097152
GenL4.menu.pnum.GENERIC_L4S9ZITX.upload.maximum_data_size=655360
GenL4.menu.pnum.GENERIC_L4S9ZITX.build.board=GENERIC_L4S9ZITX
GenL4.menu.pnum.GENERIC_L4S9ZITX.build.product_line=STM32L4S9xx
GenL4.menu.pnum.GENERIC_L4S9ZITX.build.variant=STM32L4xx/L4R9Z(G-I)T_L4S9ZIT
GenL4.menu.pnum.GENERIC_L4S9ZITX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32L4xx/STM32L4S9.svd

