# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic WL54JCIx
GenWL.menu.pnum.GENERIC_WL54JCIX=Generic WL54JCIx
GenWL.menu.pnum.GENERIC_WL54JCIX.upload.maximum_size=262144
GenWL.menu.pnum.GENERIC_WL54JCIX.upload.maximum_data_size=65536
GenWL.menu.pnum.GENERIC_WL54JCIX.build.board=GENERIC_WL54JCIX
GenWL.menu.pnum.GENERIC_WL54JCIX.build.product_line=STM32WL54xx
GenWL.menu.pnum.GENERIC_WL54JCIX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WL54JCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WL5x_CM4.svd

# Generic WL55JCIx
GenWL.menu.pnum.GENERIC_WL55JCIX=Generic WL55JCIx
GenWL.menu.pnum.GENERIC_WL55JCIX.upload.maximum_size=262144
GenWL.menu.pnum.GENERIC_WL55JCIX.upload.maximum_data_size=65536
GenWL.menu.pnum.GENERIC_WL55JCIX.build.board=GENERIC_WL55JCIX
GenWL.menu.pnum.GENERIC_WL55JCIX.build.product_line=STM32WL55xx
GenWL.menu.pnum.GENERIC_WL55JCIX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WL55JCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WL5x_CM4.svd

# Generic WLE4J8Ix
GenWL.menu.pnum.GENERIC_WLE4J8IX=Generic WLE4J8Ix
GenWL.menu.pnum.GENERIC_WLE4J8IX.upload.maximum_size=65536
GenWL.menu.pnum.GENERIC_WLE4J8IX.upload.maximum_data_size=20480
GenWL.menu.pnum.GENERIC_WLE4J8IX.build.board=GENERIC_WLE4J8IX
GenWL.menu.pnum.GENERIC_WLE4J8IX.build.product_line=STM32WLE4xx
GenWL.menu.pnum.GENERIC_WLE4J8IX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WLE4J8IX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WLE5_CM4.svd

# Generic WLE4JBIx
GenWL.menu.pnum.GENERIC_WLE4JBIX=Generic WLE4JBIx
GenWL.menu.pnum.GENERIC_WLE4JBIX.upload.maximum_size=131072
GenWL.menu.pnum.GENERIC_WLE4JBIX.upload.maximum_data_size=49152
GenWL.menu.pnum.GENERIC_WLE4JBIX.build.board=GENERIC_WLE4JBIX
GenWL.menu.pnum.GENERIC_WLE4JBIX.build.product_line=STM32WLE4xx
GenWL.menu.pnum.GENERIC_WLE4JBIX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WLE4JBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WLE5_CM4.svd

# Generic WLE4JCIx
GenWL.menu.pnum.GENERIC_WLE4JCIX=Generic WLE4JCIx
GenWL.menu.pnum.GENERIC_WLE4JCIX.upload.maximum_size=262144
GenWL.menu.pnum.GENERIC_WLE4JCIX.upload.maximum_data_size=65536
GenWL.menu.pnum.GENERIC_WLE4JCIX.build.board=GENERIC_WLE4JCIX
GenWL.menu.pnum.GENERIC_WLE4JCIX.build.product_line=STM32WLE4xx
GenWL.menu.pnum.GENERIC_WLE4JCIX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WLE4JCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WLE5_CM4.svd

# Generic WLE5J8Ix
GenWL.menu.pnum.GENERIC_WLE5J8IX=Generic WLE5J8Ix
GenWL.menu.pnum.GENERIC_WLE5J8IX.upload.maximum_size=65536
GenWL.menu.pnum.GENERIC_WLE5J8IX.upload.maximum_data_size=20480
GenWL.menu.pnum.GENERIC_WLE5J8IX.build.board=GENERIC_WLE5J8IX
GenWL.menu.pnum.GENERIC_WLE5J8IX.build.product_line=STM32WLE5xx
GenWL.menu.pnum.GENERIC_WLE5J8IX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WLE5J8IX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WLE5_CM4.svd

# Generic WLE5JBIx
GenWL.menu.pnum.GENERIC_WLE5JBIX=Generic WLE5JBIx
GenWL.menu.pnum.GENERIC_WLE5JBIX.upload.maximum_size=131072
GenWL.menu.pnum.GENERIC_WLE5JBIX.upload.maximum_data_size=49152
GenWL.menu.pnum.GENERIC_WLE5JBIX.build.board=GENERIC_WLE5JBIX
GenWL.menu.pnum.GENERIC_WLE5JBIX.build.product_line=STM32WLE5xx
GenWL.menu.pnum.GENERIC_WLE5JBIX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WLE5JBIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WLE5_CM4.svd

# Generic WLE5JCIx
GenWL.menu.pnum.GENERIC_WLE5JCIX=Generic WLE5JCIx
GenWL.menu.pnum.GENERIC_WLE5JCIX.upload.maximum_size=262144
GenWL.menu.pnum.GENERIC_WLE5JCIX.upload.maximum_data_size=65536
GenWL.menu.pnum.GENERIC_WLE5JCIX.build.board=GENERIC_WLE5JCIX
GenWL.menu.pnum.GENERIC_WLE5JCIX.build.product_line=STM32WLE5xx
GenWL.menu.pnum.GENERIC_WLE5JCIX.build.variant=STM32WLxx/WL54JCI_WL55JCI_WLE4J(8-B-C)I_WLE5J(8-B-C)I
GenWL.menu.pnum.GENERIC_WLE5JCIX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WLxx/STM32WLE5_CM4.svd

