# This file help to add generic board entry.
# upload.maximum_size and product_line have to be verified
# and changed if needed.
# See: https://github.com/stm32duino/Arduino_Core_STM32/wiki/Add-a-new-variant-%28board%29

# Generic WB55VCQx
GenWB.menu.pnum.GENERIC_WB55VCQX=Generic WB55VCQx
GenWB.menu.pnum.GENERIC_WB55VCQX.upload.maximum_size=262144
GenWB.menu.pnum.GENERIC_WB55VCQX.upload.maximum_data_size=131072
GenWB.menu.pnum.GENERIC_WB55VCQX.build.board=GENERIC_WB55VCQX
GenWB.menu.pnum.GENERIC_WB55VCQX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55VCQX.build.variant=STM32WBxx/WB55V(C-E-G)(Q-Y)_WB55VYY
GenWB.menu.pnum.GENERIC_WB55VCQX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55VCYx
GenWB.menu.pnum.GENERIC_WB55VCYX=Generic WB55VCYx
GenWB.menu.pnum.GENERIC_WB55VCYX.upload.maximum_size=262144
GenWB.menu.pnum.GENERIC_WB55VCYX.upload.maximum_data_size=131072
GenWB.menu.pnum.GENERIC_WB55VCYX.build.board=GENERIC_WB55VCYX
GenWB.menu.pnum.GENERIC_WB55VCYX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55VCYX.build.variant=STM32WBxx/WB55V(C-E-G)(Q-Y)_WB55VYY
GenWB.menu.pnum.GENERIC_WB55VCYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55VEQx
GenWB.menu.pnum.GENERIC_WB55VEQX=Generic WB55VEQx
GenWB.menu.pnum.GENERIC_WB55VEQX.upload.maximum_size=524288
GenWB.menu.pnum.GENERIC_WB55VEQX.upload.maximum_data_size=262144
GenWB.menu.pnum.GENERIC_WB55VEQX.build.board=GENERIC_WB55VEQX
GenWB.menu.pnum.GENERIC_WB55VEQX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55VEQX.build.variant=STM32WBxx/WB55V(C-E-G)(Q-Y)_WB55VYY
GenWB.menu.pnum.GENERIC_WB55VEQX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55VEYx
GenWB.menu.pnum.GENERIC_WB55VEYX=Generic WB55VEYx
GenWB.menu.pnum.GENERIC_WB55VEYX.upload.maximum_size=524288
GenWB.menu.pnum.GENERIC_WB55VEYX.upload.maximum_data_size=262144
GenWB.menu.pnum.GENERIC_WB55VEYX.build.board=GENERIC_WB55VEYX
GenWB.menu.pnum.GENERIC_WB55VEYX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55VEYX.build.variant=STM32WBxx/WB55V(C-E-G)(Q-Y)_WB55VYY
GenWB.menu.pnum.GENERIC_WB55VEYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55VGQx
GenWB.menu.pnum.GENERIC_WB55VGQX=Generic WB55VGQx
GenWB.menu.pnum.GENERIC_WB55VGQX.upload.maximum_size=1048576
GenWB.menu.pnum.GENERIC_WB55VGQX.upload.maximum_data_size=262144
GenWB.menu.pnum.GENERIC_WB55VGQX.build.board=GENERIC_WB55VGQX
GenWB.menu.pnum.GENERIC_WB55VGQX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55VGQX.build.variant=STM32WBxx/WB55V(C-E-G)(Q-Y)_WB55VYY
GenWB.menu.pnum.GENERIC_WB55VGQX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55VGYx
GenWB.menu.pnum.GENERIC_WB55VGYX=Generic WB55VGYx
GenWB.menu.pnum.GENERIC_WB55VGYX.upload.maximum_size=1048576
GenWB.menu.pnum.GENERIC_WB55VGYX.upload.maximum_data_size=262144
GenWB.menu.pnum.GENERIC_WB55VGYX.build.board=GENERIC_WB55VGYX
GenWB.menu.pnum.GENERIC_WB55VGYX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55VGYX.build.variant=STM32WBxx/WB55V(C-E-G)(Q-Y)_WB55VYY
GenWB.menu.pnum.GENERIC_WB55VGYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

# Generic WB55VYYx
GenWB.menu.pnum.GENERIC_WB55VYYX=Generic WB55VYYx
GenWB.menu.pnum.GENERIC_WB55VYYX.upload.maximum_size=655360
GenWB.menu.pnum.GENERIC_WB55VYYX.upload.maximum_data_size=262144
GenWB.menu.pnum.GENERIC_WB55VYYX.build.board=GENERIC_WB55VYYX
GenWB.menu.pnum.GENERIC_WB55VYYX.build.product_line=STM32WB55xx
GenWB.menu.pnum.GENERIC_WB55VYYX.build.variant=STM32WBxx/WB55V(C-E-G)(Q-Y)_WB55VYY
GenWB.menu.pnum.GENERIC_WB55VYYX.debug.svd_file={runtime.tools.STM32_SVD.path}/svd/STM32WBxx/STM32WB55_CM4.svd

