# Dimension, end-time (years) and output directory
# Only does zeroth time-step to show that initial condition works

set Dimension                              = 2
set Use years in output instead of seconds = true
set Start time                             = 0
set End time                               = 0

# If you have a large model or a model with large viscosity variation and you
# want to run the 0th timestep more quickly in order to just check in the initial
# condition (IC), you can set these solver tolerance values to larger numbers, but
# this means the solution will not be converged.

subsection Solver parameters
  subsection Stokes solver parameters
    set Linear solver tolerance            = 1e-6 # can set to 1e-3 for checking IC
  end
end
