
Clover EFI installer log - Thu Aug  8 15:28:34 CST 2019
Installer version: v2.5k r5038 EFI bootloader
======================================================
Changes:
Mount ESP Beta (r5030): use of a new command line called espfinder to find the ESP that belong with the target volume
using the installer. espfinder is able to find the ESP for standard hfs fylesystem, APFS, CoreStorage, RAID with or without APFS,
Fusion drives... or combined. Is in beta stage and is not used by default, in fact to activate it you have to create a file in "/"
called useespfinder just before running the installer:
sudo touch /useespfinder

- New Drivers directories (r4986): drivers64 and drivers64UEFI are deprecated and now Clover load drivers from
EFI/CLOVER/drivers/BIOS and EFI/CLOVER/drivers/UEFI. The Installer takes the step for the migration without, however,
deleting old directories. Anyway the installers now only update EFI/CLOVER/drivers/ leaving old path untouched.
For retro compatibility new Clover loads drivers from drivers64/drivers64UEFI only if EFI/CLOVER/drivers/(BIOS or UEFI)
are not present. You can safely remove drivers64 and drivers64UEFI using newer revisions.
Additionally, during the migration each driver with the "-64" suffix will be renamed without it.. as Clover is for some
time 64-bit only. None of the mentioned changes affect any functionality

- Conflicting drivers:
VirtualSMC.efi is removed if SMCHelper.efi is selected.
HFSPlus.efi is removed if VBoxHfs.efi is selected or viceversa.
ApfsDriverLoader.efi is removed if apfs.efi is selected or viceversa.
Only one of OsxAptioFixDrv.efi, OsxAptioFix3Drv.efi, AptioMemoryFix.efi, OsxLowMemFixDrv.efi is allowed
and any driver that match with "aptiofix", "memfix" or "memoryfix" will be deleted.

- Drivers off (r4987): installs all drivers available in EFI/CLOVER/drivers/off. This path is ignored by Clover and is only
used as a repository, e.g., if you want move a driver using the EFI Shell or the Finder.

A backup is always made to the root of the target volume.


======================================================
/dev/disk0 (internal):
   #:                       TYPE NAME                    SIZE       IDENTIFIER
   0:      GUID_partition_scheme                         500.1 GB   disk0
   1:                        EFI EFI                     209.7 MB   disk0s1
   2:                 Apple_APFS Container disk1         499.9 GB   disk0s2

/dev/disk1 (synthesized):
   #:                       TYPE NAME                    SIZE       IDENTIFIER
   0:      APFS Container Scheme -                      +499.9 GB   disk1
                                 Physical Store disk0s2
   1:                APFS Volume M2                      357.9 GB   disk1s1
   2:                APFS Volume Preboot                 45.7 MB    disk1s2
   3:                APFS Volume Recovery                510.3 MB   disk1s3
   4:                APFS Volume VM                      2.1 GB     disk1s4

using old scripting mode
Target volume /Volumes/M2 on disk1 is APFS on physical store disk0s2
ESP BSD Name is disk0s1
======================================================
Backing up EFI files

Backing up /Volumes/M2/EFIROOTDIR/EFI folder to /Volumes/M2/EFI-Backups/r5033/2019-08-08-15h28/EFI
======================================================
Installing BootSectors/BootLoader

Stage 0 - Don't write any of boot0af, boot0md, boot0ss to /
Stage 1 - Don't write any of boot1h2, boot1f32alt, boot1xalt to /
======================================================
Installing RC Scripts

Installing RC scripts on target volume '/'


======================================================
=========== Clover EFI Installation Finish ===========
======================================================
